(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 150 100)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(J1-NC-PadNC2)")
	(net 2 "unconnected-(J1-NC-PadNC1)")
	(net 3 "/BTN2")
	(net 4 "/BTN8")
	(net 5 "/BTN6")
	(net 6 "/BTN5")
	(net 7 "/BTN3")
	(net 8 "+3.3V")
	(net 9 "/BTN7")
	(net 10 "/BTN4")
	(net 11 "unconnected-(J2-NC-PadNC2)")
	(net 12 "unconnected-(J2-NC-PadNC1)")
	(net 13 "/BTN1")
	(net 14 "unconnected-(USB1-DN1-Pad7)")
	(net 15 "unconnected-(USB1-SBU2-Pad3)")
	(net 16 "unconnected-(USB1-SHIELD-Pad13)")
	(net 17 "unconnected-(USB1-CC2-Pad10)")
	(net 18 "unconnected-(USB1-GND-Pad12)")
	(net 19 "unconnected-(USB1-DP1-Pad6)")
	(net 20 "unconnected-(USB1-DP2-Pad8)")
	(net 21 "unconnected-(USB1-GND-Pad1)")
	(net 22 "unconnected-(USB1-SBU1-Pad9)")
	(net 23 "unconnected-(USB1-DN2-Pad5)")
	(net 24 "unconnected-(USB1-VBUS-Pad2)")
	(net 25 "unconnected-(USB1-CC1-Pad4)")
	(net 26 "unconnected-(USB1-VBUS-Pad11)")
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "0dd24026-2f52-4b3e-ac16-14c99cceb3ef")
		(at 231.45 50.68)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN2"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "d450526c-770a-45fb-9929-c015886f2523")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "b5c4d203-1de4-48dd-812e-89f65db4bac5")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4447c1ab-d623-45cf-aaa8-ca850e2f6146")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80afc9a3-6f05-40d4-80b3-88ce7ecbcc0d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/661ac862-a63b-4601-8609-65d217d322df")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "86eba2f2-a0ca-4398-a9aa-ae9b17cc77b1")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 3 "/BTN2")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "012d76f8-8222-4756-b02d-2a95e191a8a3")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "add1830c-5401-4b8b-9b8c-0871fb785c64")
		)
		(embedded_fonts no)
	)
	(footprint "extern:HRO-TYPE-C-31-M-12-HandSoldering"
		(layer "F.Cu")
		(uuid "4beccd5a-a326-43a4-9a67-43900cff29f5")
		(at 256.234369 56.015814 112.5)
		(property "Reference" "USB1"
			(at -0.000001 -10.2 112.5)
			(layer "F.SilkS")
			(uuid "eeccdc21-72a1-4e24-983a-c1d11db1c45b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "HRO-TYPE-C-31-M-12"
			(at 0 1.150001 112.5)
			(layer "Dwgs.User")
			(uuid "76331ff8-8c8b-4f89-9e55-9b6145c1caf4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 112.5)
			(layer "F.Fab")
			(hide yes)
			(uuid "17d3accb-bbb8-4d56-804e-fe9cdbe42d11")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 112.5)
			(layer "F.Fab")
			(hide yes)
			(uuid "209dad48-326b-415e-9d0d-28f1b0f1061c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/bc72ddaa-2b57-4eec-afb1-1eff5b9cf74c")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.47 -7.3)
			(end 4.470001 -7.299999)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "82b49848-600f-4a4f-a21b-65f1a6eac047")
		)
		(fp_line
			(start 4.47 0)
			(end 4.470001 -7.299999)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a6000cbf-e8fe-4651-8c82-81d3d5de8198")
		)
		(fp_line
			(start -4.47 0)
			(end -4.47 -7.3)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "6fa6326d-5e34-44ce-90c4-9c23865e18d4")
		)
		(fp_line
			(start -4.47 0)
			(end 4.47 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "cfe2d823-6958-4d9c-bdbb-1f1fb916a75c")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -6.25 112.5)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "6e8409e0-da9a-4b63-a487-4d6379f0174f")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -6.25 112.5)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "b8e7cd51-0d6a-43dc-8cef-2cde7340a996")
		)
		(pad "1" smd rect
			(at -3.225 -8.195 112.5)
			(size 0.6 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(USB1-GND-Pad1)")
			(pinfunction "GND")
			(pintype "input")
			(uuid "9dcf9ee5-f3e2-4f37-8e37-82795a3465e6")
		)
		(pad "2" smd rect
			(at -2.450001 -8.195 112.5)
			(size 0.6 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(USB1-VBUS-Pad2)")
			(pinfunction "VBUS")
			(pintype "input")
			(uuid "ccfdc428-6500-49b5-a407-1969c2f1c277")
		)
		(pad "3" smd rect
			(at -1.75 -8.195 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(USB1-SBU2-Pad3)")
			(pinfunction "SBU2")
			(pintype "input")
			(uuid "1d193756-2c8d-4021-9b0d-c57c74e7dd6b")
		)
		(pad "4" smd rect
			(at -1.250001 -8.195 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(USB1-CC1-Pad4)")
			(pinfunction "CC1")
			(pintype "input")
			(uuid "f2ac0a76-89e5-4c3d-b949-2ce339744a0b")
		)
		(pad "5" smd rect
			(at -0.75 -8.195 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(USB1-DN2-Pad5)")
			(pinfunction "DN2")
			(pintype "input")
			(uuid "c17e75b3-cbae-460e-9de6-c1dd4c5e6929")
		)
		(pad "6" smd rect
			(at -0.25 -8.194999 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(USB1-DP1-Pad6)")
			(pinfunction "DP1")
			(pintype "input")
			(uuid "61f7e806-7262-4eb0-942a-fa35ecbdee47")
		)
		(pad "7" smd rect
			(at 0.250001 -8.195 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(USB1-DN1-Pad7)")
			(pinfunction "DN1")
			(pintype "input")
			(uuid "107dc11e-9288-414e-9d5b-2e44af834a1a")
		)
		(pad "8" smd rect
			(at 0.75 -8.195 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(USB1-DP2-Pad8)")
			(pinfunction "DP2")
			(pintype "input")
			(uuid "7b959085-0bd2-4941-a91e-26896413d2ff")
		)
		(pad "9" smd rect
			(at 1.25 -8.195001 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(USB1-SBU1-Pad9)")
			(pinfunction "SBU1")
			(pintype "input")
			(uuid "a30c5ece-2c89-4d4c-a619-bd4b671d9da7")
		)
		(pad "10" smd rect
			(at 1.750001 -8.195 112.5)
			(size 0.3 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(USB1-CC2-Pad10)")
			(pinfunction "CC2")
			(pintype "input")
			(uuid "3bdcbcc0-6a9c-4574-8eb4-fb78f971084c")
		)
		(pad "11" smd rect
			(at 2.450001 -8.195 112.5)
			(size 0.6 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(USB1-VBUS-Pad11)")
			(pinfunction "VBUS")
			(pintype "input")
			(uuid "fbd9c055-95f9-4ccd-8eb8-dba7cf125cae")
		)
		(pad "12" smd rect
			(at 3.224999 -8.195 112.5)
			(size 0.6 2.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(USB1-GND-Pad12)")
			(pinfunction "GND")
			(pintype "input")
			(uuid "53ddd45f-d427-4419-941c-c32bb5360d84")
		)
		(pad "13" thru_hole oval
			(at -4.320001 -2.6 112.5)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "B.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(USB1-SHIELD-Pad13)")
			(pinfunction "SHIELD")
			(pintype "input")
			(uuid "652ce209-6df1-4901-a868-48d18a094d82")
		)
		(pad "13" thru_hole oval
			(at -4.32 -6.78 112.5)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "B.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(USB1-SHIELD-Pad13)")
			(pinfunction "SHIELD")
			(pintype "input")
			(uuid "cc25f18f-c111-4301-8993-fac3e3fd2ca0")
		)
		(pad "13" thru_hole oval
			(at 4.32 -6.78 112.5)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "B.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(USB1-SHIELD-Pad13)")
			(pinfunction "SHIELD")
			(pintype "input")
			(uuid "6270735b-a217-40f3-883a-a5860e2773bf")
		)
		(pad "13" thru_hole oval
			(at 4.32 -2.6 112.5)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "B.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(USB1-SHIELD-Pad13)")
			(pinfunction "SHIELD")
			(pintype "input")
			(uuid "2cf8a390-5bed-4762-84e2-f762ce318ee3")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "6a77e31b-8601-446e-b5fe-9c22d063d94e")
		(at 237.25 47.98)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN5"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "76f53d7e-c23a-427f-b970-ec8f1f4e6338")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "2d08336b-e645-44f3-b664-585d31b1b0c1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ba6f0b0-695d-48fc-a591-64dd37616a55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b98f19a1-38e3-4fea-a80c-e668d58215e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/5126b902-b93c-43d9-ade8-4f5d332c240a")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "59b94c3a-226a-4ffe-806b-8d70cc4c5d84")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 6 "/BTN5")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "4881874d-1f92-4e9d-b702-050ba0441a0f")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "cb9c1ffa-55ff-4350-b7ff-cdbb96204946")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_SparkFun-Connector:JST_1x08_P1.25mm_Locking_Horizontal_SMD"
		(layer "F.Cu")
		(uuid "a7a2d7b6-397e-44a4-84ba-00d07e3b72dd")
		(at 228.103657 38.45 -140)
		(tags "SparkFun")
		(property "Reference" "J1"
			(at 0 0 40)
			(layer "F.Fab")
			(uuid "fb9a713e-c7f2-4def-b6d2-de1dace74017")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Input"
			(at -0.000001 0.9 40)
			(layer "F.Fab")
			(uuid "adf6646a-2fa4-4c7f-b6b7-0acdcdde81b6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
			(at 0.000001 1.700001 220)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "548c7f5a-fec9-4c7c-930c-b10368f977b6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(property "Description" "JST locking connector"
			(at -2.500001 1.55 220)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "474116bf-7f22-4750-8cf5-a761cafa2701")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "PROD_ID" "CONN-25026"
			(at 0 0 220)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f577c948-987b-4e74-bce8-05fbddd6a7ce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/14639785-8e13-4ae1-9ff3-b7b53bf5bca1")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr smd)
		(fp_line
			(start 6.549999 -0.45)
			(end 6.55 -1.4)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9118844b-e1a5-4dc9-b353-23427c587ec4")
		)
		(fp_line
			(start 5.499999 -1.4)
			(end 6.55 -1.4)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9edc0ad-259c-482a-84cf-fe7d178a6870")
		)
		(fp_line
			(start -5 2.475)
			(end 5 2.474999)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45755f1f-fc0c-40b4-8656-86f7db8a7e7b")
		)
		(fp_line
			(start -6.55 -0.45)
			(end -6.55 -1.4)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68432940-2721-4e9e-bb93-dad04a1fec38")
		)
		(fp_line
			(start -6.55 -1.4)
			(end -5.5 -1.4)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd42b2b9-6dcd-4a61-95a6-045e65d1c96c")
		)
		(fp_poly
			(pts
				(xy 6.85 2.899999) (xy -6.85 2.899999) (xy -6.849999 -2.700001) (xy 6.85 -2.7)
			)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "0f63722c-893a-47f0-a266-aa0aa7ae51aa")
		)
		(fp_poly
			(pts
				(xy 6.125 2.549999) (xy 6.325001 2.55) (xy 6.325 0.35) (xy 6.125 0.349999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "abf8ac02-25af-4442-974d-7666136c84c9")
		)
		(fp_poly
			(pts
				(xy 4.275 -1.500001) (xy 4.475 -1.5) (xy 4.474999 -2.3) (xy 4.275 -2.299999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "7448a0e4-d4a2-4d67-8ae6-ffcead393bc6")
		)
		(fp_poly
			(pts
				(xy 3.025 -1.5) (xy 3.225 -1.499999) (xy 3.225 -2.3) (xy 3.024999 -2.300001)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "42a645cb-3e5a-46d4-ab6d-a070f394a02b")
		)
		(fp_poly
			(pts
				(xy 1.775 -1.500001) (xy 1.975 -1.5) (xy 1.974999 -2.299999) (xy 1.775 -2.299999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "036b7c31-1bce-4fd6-83b6-f9246ae5aba1")
		)
		(fp_poly
			(pts
				(xy 0.524999 -1.499999) (xy 0.725 -1.499999) (xy 0.724999 -2.3) (xy 0.525 -2.300001)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "73bade1c-cc52-44d8-a468-812237ec92d2")
		)
		(fp_poly
			(pts
				(xy -0.725 -1.500001) (xy -0.525 -1.5) (xy -0.525001 -2.3) (xy -0.725 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "1d7b7fb5-598b-4359-b0bd-3af06f8c10d1")
		)
		(fp_poly
			(pts
				(xy -1.975001 -1.499999) (xy -1.775001 -1.5) (xy -1.775 -2.3) (xy -1.974999 -2.299999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "11cc1bc8-68a9-4060-9f3e-96041d4d5ccb")
		)
		(fp_poly
			(pts
				(xy -6.324999 2.55) (xy -6.125001 2.55) (xy -6.125 0.349999) (xy -6.325 0.349999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "2682fbf8-aee3-4e69-b9b3-9bfa04d69f4b")
		)
		(fp_poly
			(pts
				(xy -3.225001 -1.500001) (xy -3.024999 -1.499999) (xy -3.025001 -2.300001) (xy -3.225 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "6bf75118-93bf-486a-b24d-4c70b230686d")
		)
		(fp_poly
			(pts
				(xy -4.475 -1.499999) (xy -4.275001 -1.5) (xy -4.274999 -2.3) (xy -4.474998 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "07538fbe-8cd8-4b5f-8a2f-5326584f3797")
		)
		(fp_poly
			(pts
				(xy -5.625 -0.3) (xy 5.625001 -0.300001) (xy 5.624999 5.4) (xy -5.625 5.400001)
			)
			(stroke
				(width 0.01)
				(type default)
			)
			(fill no)
			(layer "User.1")
			(uuid "fcb9b2f0-f5a7-460d-bdd6-d399304040e6")
		)
		(fp_poly
			(pts
				(xy -6.625001 -1.5) (xy 6.624999 -1.500001) (xy 6.625 2.550001) (xy -6.625 2.55)
			)
			(stroke
				(width 0.01)
				(type default)
			)
			(fill no)
			(layer "User.1")
			(uuid "c51a5e30-b6e9-49cf-8bef-fcc8a48495e4")
		)
		(fp_text user "Connector"
			(at -0.000001 4.349999 220)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "222b8cef-f052-47cb-aed2-77ba7da1e1e8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "Mating"
			(at 0 3.725 220)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c6d40070-3dd9-456e-b36b-58379ddf61ce")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(pad "1" smd rect
			(at -4.375 -1.750001 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "b683163f-9e82-464d-bdbd-bff8578db151")
		)
		(pad "2" smd rect
			(at -3.125 -1.749999 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/BTN2")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "1601a0a5-e5de-43ab-9801-c02d9e356998")
		)
		(pad "3" smd rect
			(at -1.874999 -1.75 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/BTN3")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "808572cc-5601-4584-9737-6b9f06a5d9d3")
		)
		(pad "4" smd rect
			(at -0.625 -1.750001 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/BTN4")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "e6c30bc3-b068-43eb-8253-a17f83296ab7")
		)
		(pad "5" smd rect
			(at 0.625001 -1.75 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/BTN5")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "68b55641-a90a-4f72-a846-8ac2a422553c")
		)
		(pad "6" smd rect
			(at 1.875 -1.75 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/BTN6")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "68809999-2605-48ff-9092-3d1669f0ead6")
		)
		(pad "7" smd rect
			(at 3.125 -1.75 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/BTN7")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "d67db083-cc8d-4b85-b983-717a47f25b52")
		)
		(pad "8" smd rect
			(at 4.375 -1.75 220)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/BTN8")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "31665159-f52e-4e50-8295-a5c6f20f63f0")
		)
		(pad "NC1" smd rect
			(at -6.225002 1.45 220)
			(size 1 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "unconnected-(J1-NC-PadNC1)")
			(pinfunction "NC")
			(pintype "no_connect")
			(thermal_bridge_angle 0)
			(uuid "a7c0bad3-649e-48d6-815b-520f31702436")
		)
		(pad "NC2" smd rect
			(at 6.225 1.450001 220)
			(size 1 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "unconnected-(J1-NC-PadNC2)")
			(pinfunction "NC")
			(pintype "no_connect")
			(thermal_bridge_angle 0)
			(uuid "10ec0e72-5964-41a8-8d70-1dc02563a375")
		)
		(embedded_fonts no)
		(model "${KICAD9_3RD_PARTY}/3dmodels/com_github_sparkfun_SparkFun-KiCad-Libraries/Connector.3dshapes/JST_SMD_1.25mm-8_Locking.step"
			(offset
				(xyz -3.75 -0.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "c4968e4d-a144-48ee-a6bd-51db0c573e4f")
		(at 234.35 47.98)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN3"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "44db893b-3f33-4b65-8a89-06656dce3c51")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "d995f210-f266-46d5-af6e-ca73963e8b23")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "239b13c9-ddfe-4d44-93b3-6c9e351aadcc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0630ee9-b1c2-4ecc-a618-1251c16b8e83")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/63539d33-ac19-4636-a8ca-eb796cc007cb")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "14ac6c30-6c23-4d40-9423-8cf483a010d4")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 7 "/BTN3")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "6964e870-e6dc-48b3-80a0-3ec54d09734f")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "8726d3eb-441f-4d12-9676-d2ea127b4f77")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "db9f2ec9-09d3-480b-a7ca-e3a9cd69cef2")
		(at 237.25 50.68)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN6"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "648092a8-9b2b-4418-87b9-0b820bfdc8ba")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "b5cb0974-fa09-4ad1-a6c4-77a66034dca2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "236d1e47-664f-4053-9127-7b1c36fb40e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b01dd10b-480d-4a72-82b5-0ad0f6910c22")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/5bcc9b70-4862-43d6-b547-60744d744223")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ec81c2ef-e4ee-4e0c-a2d1-d5f46f635d95")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 5 "/BTN6")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "764ca833-ec35-4cf4-a207-5b93ffa55d03")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "8526aab9-8806-45df-a95e-87d09c814873")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_SparkFun-Connector:JST_1x08_P1.25mm_Locking_Horizontal_SMD"
		(layer "F.Cu")
		(uuid "e10586b0-78c1-4d55-b7a1-d3f40e9889fb")
		(at 247.758715 88.225 5)
		(tags "SparkFun")
		(property "Reference" "J2"
			(at 0 0 5)
			(layer "F.Fab")
			(uuid "56af6773-0d56-4692-b4a9-2f57e8da4441")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Output"
			(at 0 0.900001 5)
			(layer "F.Fab")
			(uuid "bfe70a12-1248-407f-a6ff-3acff25854c8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
			(at -0.000001 1.699999 5)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "851e1e2d-ce12-4ce5-b53f-ae2a5168e19e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(property "Description" "JST locking connector"
			(at -2.5 1.550001 5)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d0d9673b-9340-4458-9ead-164936d50617")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "PROD_ID" "CONN-25026"
			(at 0 0 5)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "707703dd-7af7-4d74-b1c4-1619c9e9ad2e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/338ff0c2-5a78-479c-95b2-f668b87e2bd2")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr smd)
		(fp_line
			(start -6.55 -1.4)
			(end -5.499999 -1.400001)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "492d627b-918f-4d04-a010-e2d6b9324de7")
		)
		(fp_line
			(start -6.55 -0.449999)
			(end -6.55 -1.4)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47c3665c-ce28-4fc5-a00a-7b57c03a3dc1")
		)
		(fp_line
			(start -5.000001 2.474999)
			(end 5.000001 2.475)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e299f9a0-2700-40de-a869-53bb005831bb")
		)
		(fp_line
			(start 5.5 -1.4)
			(end 6.550001 -1.4)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d06b654-22b2-4752-841f-a7ac07fd939c")
		)
		(fp_line
			(start 6.55 -0.450001)
			(end 6.550001 -1.4)
			(stroke
				(width 0.2032)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "849044cd-70b9-463a-a67e-b6f0fc6ed2dd")
		)
		(fp_poly
			(pts
				(xy 6.85 2.9) (xy -6.849999 2.9) (xy -6.850001 -2.7) (xy 6.85 -2.7)
			)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "4a6f1b02-8725-45a1-a47b-ea6ea9672e67")
		)
		(fp_poly
			(pts
				(xy -6.325 2.550001) (xy -6.125 2.55) (xy -6.124999 0.350001) (xy -6.325 0.349999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "4a1bd61a-3dff-40d2-9fdf-712887c98797")
		)
		(fp_poly
			(pts
				(xy -4.475 -1.500001) (xy -4.275 -1.500001) (xy -4.274999 -2.300001) (xy -4.475 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "6eb73a8d-398d-469c-980d-220d25fcee0d")
		)
		(fp_poly
			(pts
				(xy -3.224999 -1.5) (xy -3.025 -1.5) (xy -3.024999 -2.299999) (xy -3.225001 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "a3257275-fcff-44be-a35a-4ea78466c0d9")
		)
		(fp_poly
			(pts
				(xy -1.975001 -1.500001) (xy -1.775 -1.499999) (xy -1.775 -2.300001) (xy -1.974998 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "dd2da21c-e300-4ceb-abf1-f8d3a40cced9")
		)
		(fp_poly
			(pts
				(xy -0.725 -1.5) (xy -0.525 -1.500001) (xy -0.525 -2.299999) (xy -0.725 -2.300001)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "31649bc9-01b0-4f4a-9eb3-f18da76dc3ce")
		)
		(fp_poly
			(pts
				(xy 0.524999 -1.5) (xy 0.725 -1.5) (xy 0.725 -2.3) (xy 0.525 -2.299999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "ba333203-a81c-478e-93d1-2350d6c857f0")
		)
		(fp_poly
			(pts
				(xy 1.775 -1.500001) (xy 1.975 -1.5) (xy 1.975001 -2.3) (xy 1.775 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "a040c740-1287-4690-9c3d-92eb4e867476")
		)
		(fp_poly
			(pts
				(xy 3.025 -1.5) (xy 3.225001 -1.5) (xy 3.224999 -2.3) (xy 3.025 -2.299999)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "0f4a2358-4d8a-439a-bb46-29b75eeea970")
		)
		(fp_poly
			(pts
				(xy 4.275 -1.5) (xy 4.474999 -1.500001) (xy 4.475001 -2.299998) (xy 4.275001 -2.3)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "8b0bbeb6-8989-47ca-809d-41595cda5260")
		)
		(fp_poly
			(pts
				(xy 6.124999 2.55) (xy 6.325001 2.550001) (xy 6.325 0.350001) (xy 6.125001 0.35)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "10eb5a12-c0f8-44a4-9b7e-f296ae5dc614")
		)
		(fp_poly
			(pts
				(xy -6.625 -1.5) (xy 6.625001 -1.499999) (xy 6.625 2.55) (xy -6.624999 2.550001)
			)
			(stroke
				(width 0.01)
				(type default)
			)
			(fill no)
			(layer "User.1")
			(uuid "ccb94cf9-7188-4073-aacc-65daae574b67")
		)
		(fp_poly
			(pts
				(xy -5.625 -0.300001) (xy 5.625001 -0.3) (xy 5.624999 5.399999) (xy -5.625 5.4)
			)
			(stroke
				(width 0.01)
				(type default)
			)
			(fill no)
			(layer "User.1")
			(uuid "d961af1c-5489-4cca-a391-480bacdc7e91")
		)
		(fp_text user "Mating"
			(at 0.000001 3.725 5)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "013359dc-3155-42f0-bc44-28a74bb95021")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "Connector"
			(at 0.000001 4.349999 5)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "4a209683-7e0c-4366-86eb-683986441195")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(pad "1" smd rect
			(at -4.375 -1.750001 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "92a72822-d5b0-4195-b1d3-bc81870e806a")
		)
		(pad "2" smd rect
			(at -3.124999 -1.749999 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/BTN2")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "75c8f67d-bb79-411e-915f-5b1c97ca16f6")
		)
		(pad "3" smd rect
			(at -1.874999 -1.75 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/BTN3")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "8125f8f4-7a74-4733-bae5-2a1f393509cc")
		)
		(pad "4" smd rect
			(at -0.625001 -1.75 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/BTN4")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "d5473465-68a6-4261-99fc-aca651c0e5fc")
		)
		(pad "5" smd rect
			(at 0.625001 -1.750001 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/BTN5")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "ac89d96f-afd4-4f5d-aac1-c8999a951165")
		)
		(pad "6" smd rect
			(at 1.875 -1.750001 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/BTN6")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "4b9d731d-a181-4df5-a5ed-763f9eec8ce5")
		)
		(pad "7" smd rect
			(at 3.125 -1.75 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/BTN7")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "bdfee2f2-3ece-4bdf-bd70-c5d73270151c")
		)
		(pad "8" smd rect
			(at 4.375 -1.750001 5)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/BTN8")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "c583ac5a-c859-4e38-976c-9bcd8920d71c")
		)
		(pad "NC1" smd rect
			(at -6.225001 1.45 5)
			(size 1 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(J2-NC-PadNC1)")
			(pinfunction "NC")
			(pintype "no_connect")
			(thermal_bridge_angle 0)
			(uuid "2c24e496-5c22-45a2-bf7f-728f0cedc1c9")
		)
		(pad "NC2" smd rect
			(at 6.225 1.45 5)
			(size 1 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(J2-NC-PadNC2)")
			(pinfunction "NC")
			(pintype "no_connect")
			(thermal_bridge_angle 0)
			(uuid "2270f28b-4be3-4726-bcb5-1907f27a9653")
		)
		(embedded_fonts no)
		(model "${KICAD9_3RD_PARTY}/3dmodels/com_github_sparkfun_SparkFun-KiCad-Libraries/Connector.3dshapes/JST_SMD_1.25mm-8_Locking.step"
			(offset
				(xyz -3.75 -0.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "e339a2d0-e458-4a12-81ae-845de8bb1693")
		(at 240.15 50.68)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN8"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "6cad4e21-c78a-48c9-9e54-9a6710298038")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "b477da8e-afb1-4620-b7eb-90397e983d45")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "720fa883-6bcf-40a4-91e4-351f1e30286f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7fcbed3e-26a6-4de2-bae6-ed12995ac665")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/505f82df-771e-4711-998b-91fcc5ed560f")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ca961c55-4174-4174-a665-892f94061755")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 4 "/BTN8")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "b27cc68d-5e64-487e-bcfe-3e8f4c98fe31")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "0f87f25a-089c-4a0c-811b-c596ff31109d")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "ec77df68-64ae-4ef0-b63c-5a3372373960")
		(at 234.35 50.68)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN4"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "74011b41-ddb2-4bc0-a6ac-7fb25c53263f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "1eb9337f-6ed9-48c3-a77f-dacfff59b950")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "30685916-2141-47bc-b500-43a250d08eaa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "88b5b8c5-b97e-4ac6-8fcd-97e900d15bb0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/045b524f-e459-48e0-9cfe-c9db14568439")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "54656a5b-9f40-41e0-9a82-5aadf14171dd")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 10 "/BTN4")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "25ed2198-2f17-48a2-a1d2-5deded43e4f7")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "76cac8d1-eafc-49f6-9330-56aeb0ee7e86")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "efe02fab-cfb2-4708-975d-dd9bf84fa174")
		(at 231.45 47.98)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN1"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "59060754-1c7c-4b93-9635-fc76fa61bd4d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "44e18daa-f44f-46af-a498-296d2efd6926")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "690d7ef7-f12c-4a87-9b20-0e79173bb2b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e074dc6-3672-4fdc-bb56-3cb988c875a5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/7bd03311-7905-4ff8-badc-0c1d6915b4b9")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "1c1fa73f-b090-48ed-bd3e-8f0fe2849357")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "60657573-8781-45ae-9680-9ffa81cf7255")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "3153329b-93dd-4fcc-ad70-90ceae30e109")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_SparkFun-Jumper:Jumper_2_NO_NoSilk"
		(layer "F.Cu")
		(uuid "fc23c958-e03d-4708-a36a-40a5d95724fc")
		(at 240.15 47.98)
		(tags "SparkFun")
		(property "Reference" "JMP_BTN7"
			(at 0 -1.143 0)
			(layer "F.Fab")
			(uuid "87ceb7ae-adce-43bc-9059-868b7fb499ff")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify bottom)
			)
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
			(uuid "ac0ee264-9028-405e-a2c1-74191103454a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
				(justify top)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c8198913-83f3-4547-894a-ad5a9552ce0e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "23b1aa9c-3fe5-47ad-8698-a7ff5bfaeb28")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(path "/75ee6ed1-df7a-4296-ab96-8e81170f5eec")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(fp_rect
			(start -0.9 -0.8)
			(end 0.9 0.8)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "69871cab-02a5-4502-9b3a-9815901c73a5")
		)
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 9 "/BTN7")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "0f32ba74-e1af-43d8-b10f-35e1194939cb")
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 13 "/BTN1")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
			(uuid "d1015b15-ace4-4037-be84-418e7fcdc7e0")
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 217.773256 43.087472)
		(mid 231.752175 66.105577)
		(end 238.161083 92.262206)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "36df8e7f-7bfb-46b5-9767-71736a5b2056")
	)
	(gr_line
		(start 217.773256 43.087472)
		(end 233.858346 29.591077)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "4255b521-126e-4dcd-a52d-3bad88a58b2b")
	)
	(gr_line
		(start 249.20638 53.656364)
		(end 252.803139 52.159601)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "52b179c1-fd4e-4b01-b75e-1a15b41e300d")
	)
	(gr_arc
		(start 233.858346 29.591077)
		(mid 242.319868 41.121476)
		(end 249.206381 53.656364)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "668f902d-48da-48df-b490-01d37f2f6b14")
	)
	(gr_line
		(start 238.161083 92.262207)
		(end 259.086309 90.490691)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "8bd96fd5-dc4b-4ae8-984c-c188829b43f6")
	)
	(gr_circle
		(center 229.731902 42.163387)
		(end 230.781902 42.163387)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "8d2a2599-bfb1-48af-ac47-fc0e16e12636")
	)
	(gr_circle
		(center 247.278095 84.53319)
		(end 248.328095 84.53319)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "a665d3bd-b6af-419d-9379-86f35f33ce4e")
	)
	(gr_arc
		(start 252.933859 62.652034)
		(mid 256.919995 76.370263)
		(end 259.086309 90.490679)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "d7a5a0f9-417a-4cff-95e1-9ef2a9681ad2")
	)
	(gr_line
		(start 256.556614 61.20416)
		(end 252.933858 62.652034)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "edb402ba-f7e6-4370-9a85-710eb6bd68b4")
	)
	(gr_line
		(start 252.803139 52.159601)
		(end 256.556614 61.20416)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "f1a3ca09-f885-43dc-94fb-8f5752280989")
	)
	(embedded_fonts no)
)
