(module Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm (layer F.Cu) (tedit 5A0AAD30)
  (descr "PQFN 22 leads, 5x6mm, 0.127mm stencil (https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819, https://www.infineon.com/dgdl/Infineon-AN1170-AN-v05_00-EN.pdf?fileId=5546d462533600a40153559ac3e51134)")
  (tags "pqfn 22 5x6mm")
  (attr smd)
  (fp_text reference REF** (at 0 -3.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm (at 0 3.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2 -2.5) (end -3 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3.55 3.05) (end 3.55 -3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.55 3.05) (end 3.55 3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.55 -3.05) (end -3.55 3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.55 -3.05) (end -3.55 -3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3 2.5) (end -3 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3 2.5) (end -3 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3 -2.5) (end 3 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2 -2.5) (end 3 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.9 2.62) (end -0.4 2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.12 -2.62) (end 3.12 -0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.12 1.5) (end 3.12 2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.12 2.62) (end 2.8 2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.3 2.62) (end -3.12 2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.12 -2.3) (end -3.12 -2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.9 -2.62) (end -0.4 -2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.12 -2.62) (end 2.8 -2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.3 -2.62) (end -3.12 -2.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.12 2.62) (end -3.12 2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.12 -2.3) (end -3.3 -2.3) (layer F.SilkS) (width 0.12))
  (pad 10 smd rect (at 1.225 2.025) (size 2.75 0.55) (layers F.Cu F.Mask))
  (pad 10 smd rect (at 0.0625 2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad 9 smd rect (at -1.3025 2.375) (size 0.3 0.85) (layers F.Cu F.Mask))
  (pad 15 smd rect (at -1.3305 -0.05) (size 1.55 2.7) (layers F.Cu F.Mask))
  (pad 8 smd rect (at -1.9525 2.375) (size 0.3 0.85) (layers F.Cu F.Mask))
  (pad 1 smd rect (at -2.8725 -1.95) (size 0.85 0.3) (layers F.Cu F.Mask))
  (pad 4 smd rect (at -2.8725 0) (size 0.85 0.3) (layers F.Cu F.Mask))
  (pad 5 smd rect (at -2.8725 0.65) (size 0.85 0.3) (layers F.Cu F.Mask))
  (pad 6 smd rect (at -2.8725 1.3) (size 0.85 0.3) (layers F.Cu F.Mask))
  (pad 7 smd rect (at -2.8725 1.95) (size 0.85 0.3) (layers F.Cu F.Mask))
  (pad 2 smd rect (at -2.8725 -1.3) (size 0.85 0.3) (layers F.Cu F.Mask))
  (pad 3 smd rect (at -2.8725 -0.65) (size 0.85 0.3) (layers F.Cu F.Mask))
  (pad 14 smd rect (at -1.9525 -2.375) (size 0.3 0.85) (layers F.Cu F.Mask))
  (pad 13 smd rect (at -1.3025 -2.375) (size 0.3 0.85) (layers F.Cu F.Mask))
  (pad 11 smd rect (at 1.3225 0.4125) (size 2.95 1.775) (layers F.Cu F.Mask))
  (pad 11 smd rect (at 3.0475 1.15025) (size 0.5 0.2995) (layers F.Cu F.Mask))
  (pad 11 smd rect (at 3.0475 0.4125) (size 0.5 0.3) (layers F.Cu F.Mask))
  (pad 11 smd rect (at 3.0475 -0.32525) (size 0.5 0.2995) (layers F.Cu F.Mask))
  (pad 12 smd rect (at 1.223 -1.6125) (size 2.75 1.375) (layers F.Cu F.Mask))
  (pad 12 smd rect (at 0.0605 -2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad 12 smd rect (at 0.8355 -2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad 12 smd rect (at 1.6105 -2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad 12 smd rect (at 2.3855 -2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad 10 smd rect (at 0.8375 2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad 10 smd rect (at 1.6125 2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad 10 smd rect (at 2.3875 2.55) (size 0.425 0.5) (layers F.Cu F.Mask))
  (pad "" smd rect (at 0.0625 2.2205) (size 0.425 0.95) (layers F.Paste))
  (pad "" smd rect (at -1.3025 2.37) (size 0.27 0.8) (layers F.Paste))
  (pad "" smd rect (at -0.9025 -0.795) (size 0.7 1.22) (layers F.Paste))
  (pad "" smd rect (at -1.9525 2.37) (size 0.27 0.8) (layers F.Paste))
  (pad "" smd rect (at -2.8725 -1.95) (size 0.8 0.27) (layers F.Paste))
  (pad "" smd rect (at -1.9525 -2.37) (size 0.27 0.8) (layers F.Paste))
  (pad "" smd rect (at -1.3025 -2.37) (size 0.27 0.8) (layers F.Paste))
  (pad "" smd rect (at 0.4675 0.4125) (size 1.24 1.78) (layers F.Paste))
  (pad "" smd rect (at 0.5275 -1.45) (size 1.25 0.96) (layers F.Paste))
  (pad "" smd rect (at 0.0605 -2.4) (size 0.425 0.625) (layers F.Paste))
  (pad "" smd rect (at 1.8475 0.4125) (size 1.24 1.78) (layers F.Paste))
  (pad "" smd rect (at 2.9075 -0.3275) (size 0.625 0.29) (layers F.Paste))
  (pad "" smd rect (at 2.9075 1.1525) (size 0.625 0.29) (layers F.Paste))
  (pad "" smd rect (at 2.9075 0.4125) (size 0.625 0.29) (layers F.Paste))
  (pad "" smd rect (at 0.8375 2.2205) (size 0.425 0.95) (layers F.Paste))
  (pad "" smd rect (at 1.6125 2.2205) (size 0.425 0.95) (layers F.Paste))
  (pad "" smd rect (at 2.3875 2.2205) (size 0.425 0.95) (layers F.Paste))
  (pad "" smd rect (at 1.9275 -1.45) (size 1.25 0.96) (layers F.Paste))
  (pad "" smd rect (at 0.8355 -2.4) (size 0.425 0.625) (layers F.Paste))
  (pad "" smd rect (at 1.6105 -2.4) (size 0.425 0.625) (layers F.Paste))
  (pad "" smd rect (at 2.3855 -2.4) (size 0.425 0.625) (layers F.Paste))
  (pad "" smd rect (at -1.7525 -0.795) (size 0.7 1.22) (layers F.Paste))
  (pad "" smd rect (at -0.9025 0.695) (size 0.7 1.22) (layers F.Paste))
  (pad "" smd rect (at -1.7525 0.695) (size 0.7 1.22) (layers F.Paste))
  (pad "" smd rect (at -2.8725 -1.3) (size 0.8 0.27) (layers F.Paste))
  (pad "" smd rect (at -2.8725 -0.65) (size 0.8 0.27) (layers F.Paste))
  (pad "" smd rect (at -2.8725 0) (size 0.8 0.27) (layers F.Paste))
  (pad "" smd rect (at -2.8725 0.65) (size 0.8 0.27) (layers F.Paste))
  (pad "" smd rect (at -2.8725 1.3) (size 0.8 0.27) (layers F.Paste))
  (pad "" smd rect (at -2.8725 1.95) (size 0.8 0.27) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
