(module QFN-64-1EP_8x8mm_P0.4mm_EP6.5x6.5mm_ThermalVias (layer F.Cu) (tedit 5DC5F6A6)
  (descr "QFN, 64 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/64L_VQFN_8x8_with%206_5x6_5%20EP_JXX_C04-0437A.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -5.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value QFN-64-1EP_8x8mm_P0.4mm_EP6.5x6.5mm_ThermalVias (at 0 5.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.36 -4.11) (end 4.11 -4.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.11 -4.11) (end 4.11 -3.36) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.36 4.11) (end -4.11 4.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.11 4.11) (end -4.11 3.36) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.36 4.11) (end 4.11 4.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.11 4.11) (end 4.11 3.36) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.36 -4.11) (end -4.11 -4.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -3 -4) (end 4 -4) (layer F.Fab) (width 0.1))
  (fp_line (start 4 -4) (end 4 4) (layer F.Fab) (width 0.1))
  (fp_line (start 4 4) (end -4 4) (layer F.Fab) (width 0.1))
  (fp_line (start -4 4) (end -4 -3) (layer F.Fab) (width 0.1))
  (fp_line (start -4 -3) (end -3 -4) (layer F.Fab) (width 0.1))
  (fp_line (start -4.6 -4.6) (end -4.6 4.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.6 4.6) (end 4.6 4.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.6 4.6) (end 4.6 -4.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.6 -4.6) (end -4.6 -4.6) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -3.95 -3) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -3.95 -2.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -3.95 -2.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -3.95 -1.8) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -3.95 -1.4) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -3.95 -1) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -3.95 -0.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -3.95 -0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -3.95 0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -3.95 0.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -3.95 1) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -3.95 1.4) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -3.95 1.8) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at -3.95 2.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at -3.95 2.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at -3.95 3) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at -3 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at -2.6 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at -2.2 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at -1.8 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at -1.4 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at -1 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 23 smd roundrect (at -0.6 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 24 smd roundrect (at -0.2 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 25 smd roundrect (at 0.2 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 26 smd roundrect (at 0.6 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 27 smd roundrect (at 1 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 28 smd roundrect (at 1.4 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 29 smd roundrect (at 1.8 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 30 smd roundrect (at 2.2 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 31 smd roundrect (at 2.6 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 32 smd roundrect (at 3 3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 33 smd roundrect (at 3.95 3) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 34 smd roundrect (at 3.95 2.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 35 smd roundrect (at 3.95 2.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 36 smd roundrect (at 3.95 1.8) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 37 smd roundrect (at 3.95 1.4) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 38 smd roundrect (at 3.95 1) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 39 smd roundrect (at 3.95 0.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 40 smd roundrect (at 3.95 0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 41 smd roundrect (at 3.95 -0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 42 smd roundrect (at 3.95 -0.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 43 smd roundrect (at 3.95 -1) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 44 smd roundrect (at 3.95 -1.4) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 45 smd roundrect (at 3.95 -1.8) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 46 smd roundrect (at 3.95 -2.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 47 smd roundrect (at 3.95 -2.6) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 48 smd roundrect (at 3.95 -3) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 49 smd roundrect (at 3 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 50 smd roundrect (at 2.6 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 51 smd roundrect (at 2.2 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 52 smd roundrect (at 1.8 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 53 smd roundrect (at 1.4 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 54 smd roundrect (at 1 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 55 smd roundrect (at 0.6 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 56 smd roundrect (at 0.2 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 57 smd roundrect (at -0.2 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at -0.6 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 59 smd roundrect (at -1 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 60 smd roundrect (at -1.4 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 61 smd roundrect (at -1.8 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 62 smd roundrect (at -2.2 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 63 smd roundrect (at -2.6 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 64 smd roundrect (at -3 -3.95) (size 0.2 0.8) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 65 smd rect (at 0 0) (size 6.5 6.5) (layers F.Cu F.Mask))
  (pad 65 thru_hole circle (at -3 -3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -1.8 -3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -0.6 -3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 0.6 -3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 1.8 -3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 3 -3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -3 -1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -1.8 -1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -0.6 -1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 0.6 -1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 1.8 -1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 3 -1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -3 -0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -1.8 -0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -0.6 -0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 0.6 -0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 1.8 -0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 3 -0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -3 0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -1.8 0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -0.6 0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 0.6 0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 1.8 0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 3 0.6) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -3 1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -1.8 1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -0.6 1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 0.6 1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 1.8 1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 3 1.8) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -3 3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -1.8 3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at -0.6 3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 0.6 3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 1.8 3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 thru_hole circle (at 3 3) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 65 smd rect (at 0 0) (size 6.5 6.5) (layers B.Cu))
  (pad "" smd roundrect (at -2.4 -2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -2.4 -1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -2.4 0) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -2.4 1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -2.4 2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -1.2 -2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -1.2 -1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -1.2 0) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -1.2 1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at -1.2 2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 0 -2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 0 -1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 0 0) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 0 1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 0 2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 1.2 -2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 1.2 -1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 1.2 0) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 1.2 1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 1.2 2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 2.4 -2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 2.4 -1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 2.4 0) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 2.4 1.2) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (pad "" smd roundrect (at 2.4 2.4) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-64-1EP_8x8mm_P0.4mm_EP6.5x6.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)