(module Texas_R-PUQFN-N10 (layer F.Cu) (tedit 5C425719)
  (descr http://www.ti.com/general/docs/lit/getliterature.tsp?baseLiteratureNumber=MPQF186&fileType=pdf)
  (tags Texas_R-PUQFN-N10)
  (attr smd)
  (fp_text reference REF** (at 0 -2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_R-PUQFN-N10 (at 0 2.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0 270) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.03)))
  )
  (fp_line (start 0.9 -1.2) (end 0.5 -1.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.9 1.2) (end 0.5 1.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.18 1.43) (end -1.18 -1.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.18 -1.43) (end 1.18 -1.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.18 -1.43) (end 1.18 1.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.18 1.43) (end -1.18 1.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.25 -1) (end -0.75 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0.75 1) (end -0.75 1) (layer F.Fab) (width 0.1))
  (fp_line (start -0.75 1) (end -0.75 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.25 -1) (end 0.75 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 0.75 -1) (end 0.75 1) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 1.2) (end -0.9 1.2) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at -0.35 -0.75 270) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.35 0.75 270) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.35 0.75 90) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.35 -0.75 90) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.35 -0.25 90) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.35 0.25 90) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.35 0.25 270) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.35 -0.25 270) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0 -1.175 270) (size 0.63 0.35) (drill (offset 0.315 0)) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 1.175 90) (size 0.63 0.35) (drill (offset 0.315 0)) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_R-PUQFN-N10.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
