(module QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm_ThermalVias (layer F.Cu) (tedit 5DC5F6A4)
  (descr "QFN, 36 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/36L_QFN_6x6_with_3_7x3_7_EP_Punch_Dimpled_4E_C04-0241A.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -4.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm_ThermalVias (at 0 4.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.385 -3.11) (end 3.11 -3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.11 -3.11) (end 3.11 -2.385) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.385 3.11) (end -3.11 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.11 3.11) (end -3.11 2.385) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.385 3.11) (end 3.11 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.11 3.11) (end 3.11 2.385) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.385 -3.11) (end -3.11 -3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 -3) (end 3 -3) (layer F.Fab) (width 0.1))
  (fp_line (start 3 -3) (end 3 3) (layer F.Fab) (width 0.1))
  (fp_line (start 3 3) (end -3 3) (layer F.Fab) (width 0.1))
  (fp_line (start -3 3) (end -3 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -3 -2) (end -2 -3) (layer F.Fab) (width 0.1))
  (fp_line (start -3.6 -3.6) (end -3.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.6 3.6) (end 3.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.6 3.6) (end 3.6 -3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.6 -3.6) (end -3.6 -3.6) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -2.9375 -2) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -2.9375 -1.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -2.9375 -1) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -2.9375 -0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -2.9375 0) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -2.9375 0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -2.9375 1) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -2.9375 1.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -2.9375 2) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -2 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -1.5 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -1 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -0.5 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at 0 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at 0.5 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at 1 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at 1.5 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at 2 2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at 2.9375 2) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at 2.9375 1.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at 2.9375 1) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at 2.9375 0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 23 smd roundrect (at 2.9375 0) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 24 smd roundrect (at 2.9375 -0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 25 smd roundrect (at 2.9375 -1) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 26 smd roundrect (at 2.9375 -1.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 27 smd roundrect (at 2.9375 -2) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 28 smd roundrect (at 2 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 29 smd roundrect (at 1.5 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 30 smd roundrect (at 1 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 31 smd roundrect (at 0.5 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 32 smd roundrect (at 0 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 33 smd roundrect (at -0.5 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 34 smd roundrect (at -1 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 35 smd roundrect (at -1.5 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 36 smd roundrect (at -2 -2.9375) (size 0.25 0.825) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 37 smd rect (at 0 0) (size 3.7 3.7) (layers F.Cu F.Mask))
  (pad 37 thru_hole circle (at -1 -1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at 0 -1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at 1 -1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at -1 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at 1 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at -1 1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at 0 1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 thru_hole circle (at 1 1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 37 smd rect (at 0 0) (size 2.5 2.5) (layers B.Cu))
  (pad "" smd roundrect (at -0.5 -0.5) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.5 0.5) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.5 -0.5) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.5 0.5) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd custom (at -1.425 -0.5) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.269389 -0.329856) (xy 0.2087 -0.329856) (xy 0.269389 -0.269167) (xy 0.269389 0.269167)
         (xy 0.2087 0.329856) (xy -0.269389 0.329856)) (width 0.146515))
    ))
  (pad "" smd custom (at -1.425 0.5) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.269389 -0.329856) (xy 0.2087 -0.329856) (xy 0.269389 -0.269167) (xy 0.269389 0.269167)
         (xy 0.2087 0.329856) (xy -0.269389 0.329856)) (width 0.146515))
    ))
  (pad "" smd custom (at 1.425 -0.5) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.269389 -0.269167) (xy -0.2087 -0.329856) (xy 0.269389 -0.329856) (xy 0.269389 0.329856)
         (xy -0.2087 0.329856) (xy -0.269389 0.269167)) (width 0.146515))
    ))
  (pad "" smd custom (at 1.425 0.5) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.269389 -0.269167) (xy -0.2087 -0.329856) (xy 0.269389 -0.329856) (xy 0.269389 0.329856)
         (xy -0.2087 0.329856) (xy -0.269389 0.269167)) (width 0.146515))
    ))
  (pad "" smd custom (at -0.5 -1.425) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.329856 -0.269389) (xy 0.329856 -0.269389) (xy 0.329856 0.2087) (xy 0.269167 0.269389)
         (xy -0.269167 0.269389) (xy -0.329856 0.2087)) (width 0.146515))
    ))
  (pad "" smd custom (at 0.5 -1.425) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.329856 -0.269389) (xy 0.329856 -0.269389) (xy 0.329856 0.2087) (xy 0.269167 0.269389)
         (xy -0.269167 0.269389) (xy -0.329856 0.2087)) (width 0.146515))
    ))
  (pad "" smd custom (at -0.5 1.425) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.329856 -0.2087) (xy -0.269167 -0.269389) (xy 0.269167 -0.269389) (xy 0.329856 -0.2087)
         (xy 0.329856 0.269389) (xy -0.329856 0.269389)) (width 0.146515))
    ))
  (pad "" smd custom (at 0.5 1.425) (size 0.612035 0.612035) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.329856 -0.2087) (xy -0.269167 -0.269389) (xy 0.269167 -0.269389) (xy 0.329856 -0.2087)
         (xy 0.329856 0.269389) (xy -0.329856 0.269389)) (width 0.146515))
    ))
  (pad "" smd custom (at -1.425 -1.425) (size 0.601758 0.601758) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.259112 -0.259112) (xy 0.259112 -0.259112) (xy 0.259112 0.189911) (xy 0.189911 0.259112)
         (xy -0.259112 0.259112)) (width 0.167068))
    ))
  (pad "" smd custom (at -1.425 1.425) (size 0.601758 0.601758) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.259112 -0.259112) (xy 0.189911 -0.259112) (xy 0.259112 -0.189911) (xy 0.259112 0.259112)
         (xy -0.259112 0.259112)) (width 0.167068))
    ))
  (pad "" smd custom (at 1.425 -1.425) (size 0.601758 0.601758) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.259112 -0.259112) (xy 0.259112 -0.259112) (xy 0.259112 0.259112) (xy -0.189911 0.259112)
         (xy -0.259112 0.189911)) (width 0.167068))
    ))
  (pad "" smd custom (at 1.425 1.425) (size 0.601758 0.601758) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.259112 -0.189911) (xy -0.189911 -0.259112) (xy 0.259112 -0.259112) (xy 0.259112 0.259112)
         (xy -0.259112 0.259112)) (width 0.167068))
    ))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)