(module Texas_B3QFN-14-1EP_5x5.5mm_P0.65mm_ThermalVia (layer F.Cu) (tedit 5F4A4320)
  (descr "Texas instruments QFN Package, datasheet: https://www.ti.com/lit/ds/symlink/tpsm53602.pdf")
  (tags "Texas instruments QFN")
  (attr smd)
  (fp_text reference REF** (at 0 -3.65) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_B3QFN-14-1EP_5x5.5mm_P0.65mm_ThermalVia (at 0 3.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.95 3) (end -2.95 -3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.95 3) (end -2.95 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.95 -3) (end 2.95 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.95 -3) (end 2.95 -3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.5 2.85) (end -2.5 2.85) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 -2.85) (end 0 -2.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.8 -2.75) (end -2.5 -2.05) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 2.75) (end -2.5 -2.05) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 2.75) (end -2.5 2.75) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 -2.75) (end 2.5 2.75) (layer F.Fab) (width 0.1))
  (fp_line (start -1.8 -2.75) (end 2.5 -2.75) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 15 thru_hole circle (at 0 -1.9) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at 0 1.9) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at 0.95 0.95) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at -0.95 0.95) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at 0 0.95) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at 0.95 -0.95) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at -0.95 -0.95) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at 0 -0.95) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at -0.95 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 15 thru_hole circle (at 0.95 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad "" smd roundrect (at 0.425 -1.675) (size 0.6 1.15) (layers F.Paste) (roundrect_rratio 0.083)
    (zone_connect 0))
  (pad "" smd roundrect (at -0.425 1.675) (size 0.6 1.15) (layers F.Paste) (roundrect_rratio 0.083)
    (zone_connect 0))
  (pad "" smd roundrect (at -0.425 -1.675) (size 0.6 1.15) (layers F.Paste) (roundrect_rratio 0.083)
    (zone_connect 0))
  (pad "" smd roundrect (at 0.425 1.675) (size 0.6 1.15) (layers F.Paste) (roundrect_rratio 0.083)
    (zone_connect 0))
  (pad "" smd roundrect (at -0.625 -0.475) (size 0.95 0.65) (layers F.Paste) (roundrect_rratio 0.077)
    (zone_connect 0))
  (pad "" smd roundrect (at -0.625 0.475) (size 0.95 0.65) (layers F.Paste) (roundrect_rratio 0.077)
    (zone_connect 0))
  (pad "" smd roundrect (at 0.625 0.475) (size 0.95 0.65) (layers F.Paste) (roundrect_rratio 0.077)
    (zone_connect 0))
  (pad "" smd roundrect (at 0.625 -0.475) (size 0.95 0.65) (layers F.Paste) (roundrect_rratio 0.077)
    (zone_connect 0))
  (pad 15 smd custom (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask)
    (zone_connect 0)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.75 -1.25) (xy -0.75 -2.3) (xy 0.75 -2.3) (xy 0.75 -1.25)) (width 0))
      (gr_poly (pts
         (xy -0.75 1.25) (xy -0.75 2.3) (xy 0.75 2.3) (xy 0.75 1.25)) (width 0))
    ))
  (pad 15 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 13 smd roundrect (at 2.35 -1.17) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 12 smd roundrect (at 2.35 -0.52) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 11 smd roundrect (at 2.35 0.13) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 10 smd roundrect (at 2.35 0.78) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 2 smd roundrect (at -2.35 -1.17) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 3 smd roundrect (at -2.35 -0.52) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 4 smd roundrect (at -2.35 0.13) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 5 smd roundrect (at -2.35 0.78) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 9 smd roundrect (at 2.35 1.43) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 6 smd roundrect (at -2.35 1.43) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.143))
  (pad 8 smd roundrect (at 2 2.155) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1))
  (pad 7 smd roundrect (at -2 2.155) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1))
  (pad 14 smd roundrect (at 2 -2.145) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1))
  (pad 1 smd roundrect (at -2 -2.145) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_B3QFN-14-1EP_5x5.5mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
