(module WDFN-8-1EP_4x3mm_P0.65mm_EP2.4x1.8mm (layer F.Cu) (tedit 5EB11D6F)
  (descr "WDFN, 8 Pin (https://www.onsemi.com/pub/Collateral/509AF.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "WDFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.45) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value WDFN-8-1EP_4x3mm_P0.65mm_EP2.4x1.8mm (at 0 2.45) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -1.61) (end 2 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 1.61) (end 2 1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.25 -1.5) (end 2 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2 -1.5) (end 2 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2 1.5) (end -2 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2 1.5) (end -2 -0.75) (layer F.Fab) (width 0.1))
  (fp_line (start -2 -0.75) (end -1.25 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.6 -1.75) (end -2.6 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.6 1.75) (end 2.6 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.6 1.75) (end 2.6 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.6 -1.75) (end -2.6 -1.75) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -1.9 -0.975) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -1.9 -0.325) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.9 0.325) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -1.9 0.975) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 1.9 0.975) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 1.9 0.325) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 1.9 -0.325) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 1.9 -0.975) (size 0.9 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd rect (at 0 0) (size 2.4 1.8) (layers F.Cu F.Mask))
  (pad "" smd roundrect (at -0.6 -0.45) (size 0.97 0.73) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.6 0.45) (size 0.97 0.73) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.6 -0.45) (size 0.97 0.73) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.6 0.45) (size 0.97 0.73) (layers F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/WDFN-8-1EP_4x3mm_P0.65mm_EP2.4x1.8mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)