(module TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm (layer F.Cu) (tedit 5EA4C161)
  (descr "8-lead plastic dual flat, 2x3x0.75mm size, 0.5mm pitch (http://ww1.microchip.com/downloads/en/DeviceDoc/8L_TDFN_2x3_MN_C04-0129E-MN.pdf)")
  (tags "TDFN DFN 0.5mm")
  (attr smd)
  (fp_text reference REF** (at 0 -1.88) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm (at 0 1.88) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.5 -0.5) (end -1.5 1) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 1) (end 1.5 1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 1) (end 1.5 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -1) (end -1 -1) (layer F.Fab) (width 0.1))
  (fp_line (start -1 -1) (end -1.5 -0.5) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.09)))
  )
  (fp_line (start -0.45 -1.12) (end 1.45 -1.12) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.45 1.12) (end 1.45 1.12) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.13 -1.25) (end -2.13 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.13 1.25) (end 2.13 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.13 1.25) (end 2.13 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.13 -1.25) (end -2.13 -1.25) (layer F.CrtYd) (width 0.05))
  (pad 1 smd oval (at -1.45 -0.75) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -1.45 -0.25) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -1.45 0.25) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -1.45 0.75) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 1.45 -0.75) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 1.45 -0.25) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 1.45 0.25) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at 1.45 0.75) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0 0) (size 1.8 1.65) (layers F.Cu F.Mask))
  (pad "" smd rect (at 0 0) (size 1.8 0.7) (layers F.Paste))
  (pad "" smd rect (at 0 -0.5) (size 0.7 0.65) (layers F.Paste))
  (pad "" smd rect (at 0 0.5) (size 0.7 0.65) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
