(module WDFN-6-2EP_4.0x2.6mm_P0.65mm (layer F.Cu) (tedit 5F611BB7)
  (descr "WDFN, 6 pin, 4.0x2.6, 0.65P; Two exposed pads, (https://www.onsemi.com/pub/Collateral/511BZ.PDF)")
  (tags "DFN 0.65P dual flag")
  (attr smd)
  (fp_text reference REF** (at 0 -2.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value WDFN-6-2EP_4.0x2.6mm_P0.65mm (at 0 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.35 1.55) (end 2.35 1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.35 1.55) (end 2.35 -1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.35 -1.55) (end -2.35 -1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.35 -1.55) (end -2.35 1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2 -0.65) (end -1.35 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 2 -1.3) (end -1.35 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -2 -0.65) (end -2 1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -2 1.3) (end 2 1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 2 1.3) (end 2 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 2 -1.42) (end 0 -1.42) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 1.42) (end 2 1.42) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.12)))
  )
  (pad 8 smd rect (at 0 0.838 270) (size 0.615 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0 -0.438 270) (size 1.415 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.9 -0.65 270) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.9 0 270) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.9 0.65 270) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.9 0.65 270) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.9 0 270) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.9 -0.65 270) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/WDFN-6-2EP_4.0x2.6mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
