(module QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm (layer F.Cu) (tedit 5DC5F6A4)
  (descr "QFN, 32 Pin (https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf#page=108), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -4.82) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm (at 0 4.82) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.685 -3.61) (end 3.61 -3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.61 -3.61) (end 3.61 -2.685) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.685 3.61) (end -3.61 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.61 3.61) (end -3.61 2.685) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.685 3.61) (end 3.61 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.61 3.61) (end 3.61 2.685) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.685 -3.61) (end -3.61 -3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -4.12 -4.12) (end -4.12 4.12) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.12 4.12) (end 4.12 4.12) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.12 4.12) (end 4.12 -4.12) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.12 -4.12) (end -4.12 -4.12) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -3.325 -2.275) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -3.325 -1.625) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -3.325 -0.975) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -3.325 -0.325) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -3.325 0.325) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -3.325 0.975) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -3.325 1.625) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -3.325 2.275) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -2.275 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -1.625 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -0.975 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -0.325 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at 0.325 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at 0.975 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at 1.625 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at 2.275 3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at 3.325 2.275) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at 3.325 1.625) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at 3.325 0.975) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at 3.325 0.325) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at 3.325 -0.325) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at 3.325 -0.975) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 23 smd roundrect (at 3.325 -1.625) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 24 smd roundrect (at 3.325 -2.275) (size 1.1 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 25 smd roundrect (at 2.275 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 26 smd roundrect (at 1.625 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 27 smd roundrect (at 0.975 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 28 smd roundrect (at 0.325 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 29 smd roundrect (at -0.325 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 30 smd roundrect (at -0.975 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 31 smd roundrect (at -1.625 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 32 smd roundrect (at -2.275 -3.325) (size 0.3 1.1) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 33 smd rect (at 0 0) (size 4.7 4.7) (layers F.Cu F.Mask))
  (pad "" smd roundrect (at -1.77 -1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -1.77 -0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -1.77 0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -1.77 1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.59 -1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.59 -0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.59 0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.59 1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.59 -1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.59 -0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.59 0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.59 1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 1.77 -1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 1.77 -0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 1.77 0.59) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 1.77 1.77) (size 0.95 0.95) (layers F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)