(module Texas_RNN0018A (layer F.Cu) (tedit 5CACEF73)
  (descr "Texas Instruments, VQFN-HR RNN0018A (http://www.ti.com/lit/ds/symlink/tps568215.pdf)")
  (tags "ti vqfn-hr rnn0018a")
  (solder_mask_margin 0.05)
  (attr smd)
  (fp_text reference REF** (at 0 -3.175) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_RNN0018A (at 0 3.175) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.875 -1.75) (end 1.75 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 1.75 -1.75) (end 1.75 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 1.75 1.75) (end -1.75 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -1.75 1.75) (end -1.75 -0.875) (layer F.Fab) (width 0.1))
  (fp_line (start 1.57 -1.87) (end 1.87 -1.87) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.87 -1.87) (end 1.87 -1.37) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.87 1.87) (end 1.37 1.87) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.87 -1.87) (end -1.57 -1.87) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.2 -2.2) (end 2.2 -2.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.2 -2.2) (end 2.2 2.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.2 2.2) (end -2.2 2.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.2 2.2) (end -2.2 -2.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.875 -1.75) (end -1.75 -0.875) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start 1.87 1.67) (end 1.87 1.87) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.87 1.67) (end -1.87 1.87) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.87 1.87) (end -1.37 1.87) (layer F.SilkS) (width 0.12))
  (pad 1 smd roundrect (at -1.65 -0.925) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 18 smd roundrect (at -1.25 -1.65) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 16 smd roundrect (at -0.25 -1.65) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 17 smd roundrect (at -0.75 -1.65) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 12 smd roundrect (at 1.65 -0.925) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 15 smd roundrect (at 0.25 -1.65) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 14 smd roundrect (at 0.75 -1.65) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 13 smd roundrect (at 1.25 -1.65) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 2 smd roundrect (at -1.375 -0.35) (size 1.15 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.125))
  (pad 11 smd roundrect (at 1.375 -0.35) (size 1.15 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.125))
  (pad 3 smd roundrect (at -1.375 0.3) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 4 smd roundrect (at -1.375 0.85) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 5 smd roundrect (at -1.375 1.4) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 8 smd roundrect (at 1.375 1.4) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 9 smd roundrect (at 1.375 0.85) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 10 smd roundrect (at 1.375 0.3) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 6 smd roundrect (at -0.3 0.65) (size 0.3 2.6) (layers F.Cu F.Mask) (roundrect_rratio 0.166))
  (pad 7 smd roundrect (at 0.3 0.65) (size 0.3 2.6) (layers F.Cu F.Mask) (roundrect_rratio 0.166))
  (pad "" smd roundrect (at -1.375 -0.35) (size 1.15 0.36) (layers F.Paste) (roundrect_rratio 0.139))
  (pad "" smd roundrect (at 1.375 -0.35) (size 1.15 0.36) (layers F.Paste) (roundrect_rratio 0.139))
  (pad "" smd roundrect (at -0.3 -0.2825) (size 0.3 0.733) (layers F.Paste) (roundrect_rratio 0.167))
  (pad "" smd roundrect (at 0.3 0.651) (size 0.3 0.733) (layers F.Paste) (roundrect_rratio 0.167))
  (pad "" smd roundrect (at 0.3 1.585) (size 0.3 0.733) (layers F.Paste) (roundrect_rratio 0.167))
  (pad "" smd roundrect (at -0.3 1.585) (size 0.3 0.733) (layers F.Paste) (roundrect_rratio 0.167))
  (pad "" smd roundrect (at -0.3 0.651) (size 0.3 0.733) (layers F.Paste) (roundrect_rratio 0.167))
  (pad "" smd roundrect (at 0.3 -0.2825) (size 0.3 0.733) (layers F.Paste) (roundrect_rratio 0.167))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_RNN0018A.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
