(module DFN-10-1EP_2x3mm_P0.5mm_EP0.64x2.4mm (layer F.Cu) (tedit 5EA4BEAB)
  (descr "DDB Package; 10-Lead Plastic DFN (3mm x 2mm) (see Linear Technology DFN_10_05-08-1722.pdf)")
  (tags "DFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -2.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-10-1EP_2x3mm_P0.5mm_EP0.64x2.4mm (at 0 2.55) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.5 0.5) (thickness 0.075)))
  )
  (fp_line (start -0.5 -1.5) (end 1 -1.5) (layer F.Fab) (width 0.15))
  (fp_line (start 1 -1.5) (end 1 1.5) (layer F.Fab) (width 0.15))
  (fp_line (start 1 1.5) (end -1 1.5) (layer F.Fab) (width 0.15))
  (fp_line (start -1 1.5) (end -1 -1) (layer F.Fab) (width 0.15))
  (fp_line (start -1 -1) (end -0.5 -1.5) (layer F.Fab) (width 0.15))
  (fp_line (start -1.55 -1.8) (end -1.55 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.55 -1.8) (end 1.55 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.55 -1.8) (end 1.55 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.55 1.8) (end 1.55 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 1.625) (end 1 1.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -1.625) (end 1 -1.625) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -0.925 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.925 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.925 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.925 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.925 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.925 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.925 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.925 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.925 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.925 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 0) (size 0.64 2.4) (layers F.Cu F.Mask)
    (solder_paste_margin_ratio -0.2))
  (pad "" smd rect (at 0 -0.6) (size 0.5 1) (layers F.Paste))
  (pad "" smd rect (at 0 0.6) (size 0.5 1) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-10-1EP_2x3mm_P0.5mm_EP0.64x2.4mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
