(module UDFN-10_1.35x2.6mm_P0.5mm (layer F.Cu) (tedit 5EA4C1CF)
  (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/f2/11/8a/ed/40/31/40/56/DM00088292.pdf/files/DM00088292.pdf/jcr:content/translations/en.DM00088292.pdf)
  (tags "UDFN 0.5 uQFN")
  (attr smd)
  (fp_text reference REF** (at 0 -2.17) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value UDFN-10_1.35x2.6mm_P0.5mm (at 0 2.29) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0 90) (layer F.Fab)
    (effects (font (size 0.5 0.5) (thickness 0.075)))
  )
  (fp_line (start -0.3 -1.3) (end 0.675 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 0.675 -1.3) (end 0.675 1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 0.675 1.3) (end -0.675 1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -0.675 1.3) (end -0.675 -0.95) (layer F.Fab) (width 0.1))
  (fp_line (start -0.675 -0.95) (end -0.3 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -1.13 -1.55) (end -1.13 1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.13 -1.55) (end 1.13 1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.13 -1.55) (end 1.13 -1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.13 1.55) (end 1.13 1.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.65 1.4) (end 0.65 1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -1.4) (end 0.65 -1.4) (layer F.SilkS) (width 0.12))
  (pad 1 smd oval (at -0.525 -1) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -0.525 -0.5) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -0.525 0) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -0.525 0.5) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -0.525 1) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 0.525 1) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 0.525 0.5) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 0.525 0) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 0.525 -0.5) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 0.525 -1) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UDFN-10_1.35x2.6mm_P0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
