(module DFN-6_1.3x1.2mm_P0.4mm (layer F.Cu) (tedit 5A64DFC7)
  (descr "6-Lead Plastic DFN (1.3mm x 1.2mm) ")
  (tags "DFN 0.4")
  (attr smd)
  (fp_text reference REF** (at 0 -1.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-6_1.3x1.2mm_P0.4mm (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0.025) (layer F.Fab)
    (effects (font (size 0.5 0.5) (thickness 0.075)))
  )
  (fp_line (start 0 -0.7) (end 0.65 -0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.7 0.75) (end 0.65 0.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.65 0.6) (end 0.65 0.6) (layer F.Fab) (width 0.12))
  (fp_line (start 0.65 0.6) (end 0.65 -0.55) (layer F.Fab) (width 0.12))
  (fp_line (start 0.65 -0.55) (end -0.1 -0.55) (layer F.Fab) (width 0.12))
  (fp_line (start -0.1 -0.55) (end -0.65 0) (layer F.Fab) (width 0.12))
  (fp_line (start -0.65 0) (end -0.65 0.6) (layer F.Fab) (width 0.12))
  (fp_line (start -0.8 -0.7) (end 0.8 -0.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.8 -0.7) (end -0.8 0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.8 0.75) (end 0.8 -0.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.8 0.75) (end -0.8 0.75) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -0.368 -0.4) (size 0.53 0.28) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.368 0) (size 0.53 0.28) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.368 0.4) (size 0.53 0.28) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.368 0.4) (size 0.53 0.28) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.368 0) (size 0.53 0.28) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.368 -0.4) (size 0.53 0.28) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6_1.3x1.2mm_P0.4mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
