(module DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm_PullBack (layer F.Cu) (tedit 5DC5F54E)
  (descr "DFN, 6 Pin (http://www.onsemi.com/pub/Collateral/NCP133-D.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "DFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -1.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm_PullBack (at 0 1.55) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -0.71) (end 0.6 -0.71) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.6 0.71) (end 0.6 0.71) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 -0.6) (end 0.6 -0.6) (layer F.Fab) (width 0.1))
  (fp_line (start 0.6 -0.6) (end 0.6 0.6) (layer F.Fab) (width 0.1))
  (fp_line (start 0.6 0.6) (end -0.6 0.6) (layer F.Fab) (width 0.1))
  (fp_line (start -0.6 0.6) (end -0.6 -0.3) (layer F.Fab) (width 0.1))
  (fp_line (start -0.6 -0.3) (end -0.3 -0.6) (layer F.Fab) (width 0.1))
  (fp_line (start -0.85 -0.85) (end -0.85 0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.85 0.85) (end 0.85 0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.85 0.85) (end 0.85 -0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.85 -0.85) (end -0.85 -0.85) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -0.475 -0.4) (size 0.25 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -0.475 0) (size 0.25 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -0.475 0.4) (size 0.25 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 0.475 0.4) (size 0.25 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 0.475 0) (size 0.25 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 0.475 -0.4) (size 0.25 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd rect (at 0 0) (size 0.3 0.94) (layers F.Cu F.Mask))
  (pad "" smd roundrect (at 0 -0.235) (size 0.24 0.38) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0 0.235) (size 0.24 0.38) (layers F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.04)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm_PullBack.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)