(module UDFN-4-1EP_1x1mm_P0.65mm_EP0.48x0.48mm (layer F.Cu) (tedit 5C428124)
  (descr "UDFN-4_1x1mm_P0.65mm, http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550x-300mA-Single-Output-LDO-in-Small-Packages-DS20006006A.pdf")
  (tags UDFN-4_1x1mm_P0.65mm)
  (attr smd)
  (fp_text reference REF** (at 0 -1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value UDFN-4-1EP_1x1mm_P0.65mm_EP0.48x0.48mm (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.61 0.63) (end -0.61 0.63) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.9 -0.75) (end 0.9 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.9 -0.75) (end 0.9 0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.9 0.75) (end -0.9 0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.9 0.75) (end -0.9 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.12 -0.5) (end -0.5 -0.12) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 0.5) (end -0.5 0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 0.5) (end -0.5 -0.12) (layer F.Fab) (width 0.1))
  (fp_line (start -0.12 -0.5) (end 0.5 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 -0.5) (end 0.5 0.5) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0.04 0.08) (layer F.Fab)
    (effects (font (size 0.25 0.25) (thickness 0.025)))
  )
  (fp_line (start 0.61 -0.63) (end 0 -0.63) (layer F.SilkS) (width 0.12))
  (pad 4 smd custom (at 0.54 -0.325) (size 0.22 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.11 -0.125) (xy -0.29 -0.125) (xy -0.29 -0.055) (xy -0.11 0.125)) (width 0))
    ))
  (pad 1 smd custom (at -0.54 -0.325) (size 0.22 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 0.11 -0.125) (xy 0.36 -0.125) (xy 0.11 0.125)) (width 0))
    ))
  (pad 5 smd rect (at 0 0 45) (size 0.48 0.48) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd custom (at -0.54 0.325) (size 0.22 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 0.11 0.125) (xy 0.29 0.125) (xy 0.29 0.055) (xy 0.11 -0.125)) (width 0))
    ))
  (pad 3 smd custom (at 0.54 0.325) (size 0.22 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.11 0.125) (xy -0.29 0.125) (xy -0.29 0.055) (xy -0.11 -0.125)) (width 0))
    ))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UDFN-4-1EP_1x1mm_P0.65mm_EP0.48x0.48mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
