(module OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm (layer F.Cu) (tedit 5F73D1DA)
  (descr "XDFN4 footprint (as found on the https://www.onsemi.com/pub/Collateral/NCP115-D.PDF)")
  (tags "OnSemi XDFN4")
  (attr smd)
  (fp_text reference REF** (at 0.04 2.38) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm (at 0.11 -1.78) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.5 0.5) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 0.5) (end -0.5 0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 -0.5) (end 0.5 0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.25 -0.5) (end 0.5 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -0.25) (end -0.25 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.73 -0.87) (end 0.73 -0.87) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.73 -0.87) (end 0.73 0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.73 0.85) (end -0.73 0.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.73 0.85) (end -0.73 -0.87) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.72 -0.86) (end -0.3 -0.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.72 -0.3) (end -0.72 0.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.72 0.86) (end 0.72 0.86) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.72 0.86) (end 0.72 -0.86) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0.01 1.26) (layer F.Fab)
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (pad 5 smd rect (at 0 0 45) (size 0.52 0.52) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd custom (at 0.325 0.485) (size 0.26 0.23) (layers F.Cu F.Paste F.Mask)
    (zone_connect 0)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.13 -0.115) (xy 0.13 -0.115) (xy 0.13 -0.275) (xy 0.02 -0.275)) (width 0))
    ))
  (pad 2 smd custom (at 0.325 -0.485 180) (size 0.26 0.23) (layers F.Cu F.Paste F.Mask)
    (zone_connect 0)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 0.13 -0.115) (xy -0.13 -0.115) (xy -0.13 -0.275) (xy -0.02 -0.275)) (width 0))
    ))
  (pad 1 smd custom (at -0.325 -0.485 180) (size 0.26 0.23) (layers F.Cu F.Paste F.Mask)
    (zone_connect 0)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.13 -0.115) (xy 0.13 -0.115) (xy 0.13 -0.275) (xy 0.02 -0.275)) (width 0))
    ))
  (pad 4 smd custom (at -0.325 0.485) (size 0.26 0.23) (layers F.Cu F.Paste F.Mask)
    (zone_connect 0)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 0.13 -0.115) (xy -0.13 -0.115) (xy -0.13 -0.275) (xy -0.02 -0.275)) (width 0))
    ))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
