(module DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm (layer F.Cu) (tedit 5EA4BEDC)
  (descr "10-Lead Plastic Dual Flat No-Lead Package, 3x3mm Body (see Atmel Appnote 8826)")
  (tags "DFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -2.475) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm (at 0 2.475) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.105)))
  )
  (fp_line (start -2.13 -1.75) (end -2.13 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.13 -1.75) (end 2.13 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.13 1.75) (end 2.13 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.13 -1.75) (end 2.13 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -0.5) (end -0.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 1.5) (end -1.5 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -1.62) (end 1.5 -1.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 1.62) (end 1.5 1.62) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at -1.45 -1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.45 -0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.45 0) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.45 0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.45 1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.45 1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.45 0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.45 0) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.45 -0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.45 -1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 0) (size 1.75 2.7) (layers F.Cu F.Mask))
  (pad "" smd rect (at -0.3875 -0.62) (size 0.6 1.05) (layers F.Paste))
  (pad "" smd rect (at -0.3875 0.62) (size 0.6 1.05) (layers F.Paste))
  (pad "" smd rect (at 0.3875 -0.62) (size 0.6 1.05) (layers F.Paste))
  (pad "" smd rect (at 0.3875 0.62) (size 0.6 1.05) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
