(module WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm (layer F.Cu) (tedit 5DC5F6A8)
  (descr "WQFN, 14 Pin (https://www.onsemi.com/pub/Collateral/FUSB302B-D.PDF#page=32), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "WQFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm (at 0 2.55) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.135 -1.36) (end 1.36 -1.36) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.36 -1.36) (end 1.36 -0.885) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.135 1.36) (end -1.36 1.36) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.36 1.36) (end -1.36 0.885) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.135 1.36) (end 1.36 1.36) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.36 1.36) (end 1.36 0.885) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.135 -1.36) (end -1.36 -1.36) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.625 -1.25) (end 1.25 -1.25) (layer F.Fab) (width 0.1))
  (fp_line (start 1.25 -1.25) (end 1.25 1.25) (layer F.Fab) (width 0.1))
  (fp_line (start 1.25 1.25) (end -1.25 1.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 1.25) (end -1.25 -0.625) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 -0.625) (end -0.625 -1.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.85 -1.85) (end -1.85 1.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.85 1.85) (end 1.85 1.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.85 1.85) (end 1.85 -1.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.85 -1.85) (end -1.85 -1.85) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -1.2625 -0.5) (size 0.675 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -1.2625 0) (size 0.675 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.2625 0.5) (size 0.675 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -0.75 1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -0.25 1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 0.25 1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 0.75 1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 1.2625 0.5) (size 0.675 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 1.2625 0) (size 0.675 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 1.2625 -0.5) (size 0.675 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at 0.75 -1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at 0.25 -1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -0.25 -1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at -0.75 -1.2625) (size 0.25 0.675) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 15 smd rect (at 0 0) (size 1.45 1.45) (layers F.Cu F.Mask))
  (pad "" smd roundrect (at -0.36 -0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.36 0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.36 -0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.36 0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.62 0.62) (thickness 0.09)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)