(module Linear_DE14MA (layer F.Cu) (tedit 5BAD15BC)
  (descr "14-Lead Plastic DFN, 4mm x 3mm (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-dfn/05081731_C_DE14MA.pdf)")
  (tags "DFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -3.05) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Linear_DE14MA (at 0 3.05) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.1)))
  )
  (fp_line (start -1.75 -2.11) (end 1.5 -2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 2.11) (end 1.5 2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 2.25) (end 2 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2 -2.25) (end 2 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2 -2.25) (end 2 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2 -2.25) (end -2 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -1) (end -0.5 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 2) (end -1.5 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 2) (end -1.5 2) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -2) (end 1.5 2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -2) (end 1.5 -2) (layer F.Fab) (width 0.1))
  (pad 14 smd rect (at 1.4 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 1.4 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.4 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.4 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.4 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.4 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.4 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.4 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.4 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.4 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.4 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.4 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd custom (at 0 1.145) (size 1.15 1.07) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_circle (center -0.575 -0.285) (end -0.325 -0.285) (width 0))
      (gr_circle (center 0.575 -0.285) (end 0.825 -0.285) (width 0))
      (gr_circle (center -0.575 0.285) (end -0.325 0.285) (width 0))
      (gr_circle (center 0.575 0.285) (end 0.825 0.285) (width 0))
      (gr_poly (pts
         (xy -0.825 -0.285) (xy 0.825 -0.285) (xy 0.825 0.285) (xy -0.825 0.285)) (width 0))
      (gr_poly (pts
         (xy 0.825 -0.27) (xy 1.75 -0.27) (xy 1.75 -0.02) (xy 0.825 -0.02)) (width 0))
    ))
  (pad 4 smd custom (at 0 -0.79) (size 1.65 1.28) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_circle (center 0.575 -0.64) (end 0.825 -0.64) (width 0))
      (gr_circle (center 0.575 0.64) (end 0.825 0.64) (width 0))
      (gr_poly (pts
         (xy -0.575 -0.89) (xy 0.575 -0.89) (xy 0.575 0.89) (xy -0.825 0.89) (xy -0.825 -0.64)
) (width 0))
      (gr_poly (pts
         (xy -0.78 0.665) (xy -1.75 0.665) (xy -1.75 0.915) (xy -0.88 0.915) (xy -0.78 0.89)
) (width 0))
      (gr_poly (pts
         (xy -1.075 0.665) (xy -1.025 0.66) (xy -0.977 0.645) (xy -0.935 0.622) (xy -0.897 0.591)
         (xy -0.866 0.552) (xy -0.844 0.511) (xy -0.83 0.464) (xy -0.825 0.415) (xy -0.825 0.665)
) (width 0.001))
    ))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Linear_DE14MA.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
