(module DFN-14_1.35x3.5mm_P0.5mm (layer F.Cu) (tedit 5CFE70B7)
  (descr "DFN, 14 Pin (https://m.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sp3012_datasheet.pdf.pdf#page=7), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "DFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-14_1.35x3.5mm_P0.5mm (at 0 2.7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -1.86) (end 0.675 -1.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.675 1.86) (end 0.675 1.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3375 -1.75) (end 0.675 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 0.675 -1.75) (end 0.675 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start 0.675 1.75) (end -0.675 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -0.675 1.75) (end -0.675 -1.4125) (layer F.Fab) (width 0.1))
  (fp_line (start -0.675 -1.4125) (end -0.3375 -1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -1.3 -2) (end -1.3 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.3 2) (end 1.3 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.3 2) (end 1.3 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.3 -2) (end -1.3 -2) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -0.675 -1.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -0.675 -1) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -0.675 -0.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -0.675 0) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -0.675 0.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -0.675 1) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -0.675 1.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 0.675 1.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 0.675 1) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 0.675 0.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at 0.675 0) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at 0.675 -0.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at 0.675 -1) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at 0.675 -1.5) (size 0.75 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.34 0.34) (thickness 0.05)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-14_1.35x3.5mm_P0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)