(module DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm (layer F.Cu) (tedit 5EA4BFE7)
  (descr "14-lead very thin plastic quad flat, 3.0x4.5mm size, 0.65mm pitch (http://ww1.microchip.com/downloads/en/DeviceDoc/14L_VDFN_4_5x3_0mm_JHA_C041198A.pdf)")
  (tags "VDFN DFN 0.65mm")
  (attr smd)
  (fp_text reference REF** (at 0 -3.45) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm (at 0 3.65) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.5 2.35) (end 1.5 2.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.5 -2.35) (end 0 -2.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.5 -2.25) (end -0.75 -2.25) (layer F.Fab) (width 0.1))
  (fp_line (start -0.75 -2.25) (end -1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 2.25) (end -1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.75 0.75) (thickness 0.15)))
  )
  (fp_line (start -2.18 2.5) (end 2.18 2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.18 2.5) (end 2.18 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.18 -2.5) (end -2.18 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.18 -2.5) (end -2.18 2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 2.25) (end 1.5 2.25) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 2.25) (end 1.5 -2.25) (layer F.Fab) (width 0.1))
  (pad "" smd rect (at 0.4125 0.53125) (size 0.66 0.85) (layers F.Paste))
  (pad "" smd rect (at 0.4125 -0.53125) (size 0.66 0.85) (layers F.Paste))
  (pad "" smd rect (at 0.4125 1.59375) (size 0.66 0.85) (layers F.Paste))
  (pad "" smd rect (at 0.4125 -1.59375) (size 0.66 0.85) (layers F.Paste))
  (pad "" smd rect (at -0.4125 1.59375) (size 0.66 0.85) (layers F.Paste))
  (pad "" smd rect (at -0.4125 0.53125) (size 0.66 0.85) (layers F.Paste))
  (pad "" smd rect (at -0.4125 -1.59375) (size 0.66 0.85) (layers F.Paste))
  (pad 8 smd oval (at 1.5 1.95) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 1.5 1.3) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 1.5 0.65) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 1.5 0) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 1.5 -0.65) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 1.5 -1.3) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at -1.5 1.95) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at -1.5 1.3) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -1.5 0.65) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -1.5 0) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -1.5 -0.65) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -1.5 -1.3) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at 1.5 -1.95) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 0 0) (size 1.65 4.25) (layers F.Cu F.Mask))
  (pad 1 smd oval (at -1.5 -1.95) (size 0.85 0.35) (layers F.Cu F.Paste F.Mask))
  (pad "" smd rect (at -0.4125 -0.53125) (size 0.66 0.85) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-14-1EP_3x4.5mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
