(module UQFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm (layer F.Cu) (tedit 5A65CEDD)
  (descr "16-Lead Ultra Thin Quad Flat, No Lead Package (UC) - 3x3x0.5 mm Body [UQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
  (tags "QFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -2.9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value UQFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm (at 0 2.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.105)))
  )
  (fp_line (start -0.5 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.15))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.15))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.15))
  (fp_line (start -1.5 1.5) (end -1.5 -0.5) (layer F.Fab) (width 0.15))
  (fp_line (start -1.5 -0.5) (end -0.5 -1.5) (layer F.Fab) (width 0.15))
  (fp_line (start -2.15 -2.15) (end -2.15 2.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.15 -2.15) (end 2.15 2.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.15 -2.15) (end 2.15 -2.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.15 2.15) (end 2.15 2.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.65 -1.65) (end 1.65 -1.125) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.65 1.65) (end -1.65 1.125) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.65 1.65) (end 1.65 1.125) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.65 -1.65) (end -1.125 -1.65) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.65 1.65) (end -1.125 1.65) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.65 1.65) (end 1.125 1.65) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.65 -1.65) (end 1.125 -1.65) (layer F.SilkS) (width 0.15))
  (pad 1 smd oval (at -1.5 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -1.5 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -1.5 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -1.5 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -0.75 1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at -0.25 1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 0.25 1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 0.75 1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 1.5 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 1.5 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 1.5 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 1.5 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 0.75 -1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at 0.25 -1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at -0.25 -1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at -0.75 -1.5 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask))
  (pad "" smd rect (at 0.4375 0.4375) (size 0.7 0.7) (layers F.Paste))
  (pad 17 smd rect (at 0 0) (size 1.75 1.75) (layers F.Cu F.Mask))
  (pad "" smd rect (at -0.4375 0.4375) (size 0.7 0.7) (layers F.Paste))
  (pad "" smd rect (at -0.4375 -0.4375) (size 0.7 0.7) (layers F.Paste))
  (pad "" smd rect (at 0.4375 -0.4375) (size 0.7 0.7) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
