(module Texas_DRB0008A (layer F.Cu) (tedit 5CD0C7FC)
  (descr "DFN-8, 3x3x1mm, http://www.ti.com/lit/ds/symlink/ucc24610.pdf")
  (tags DRB0008A)
  (solder_mask_margin 0.07)
  (attr smd)
  (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_DRB0008A (at 0 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.1)))
  )
  (fp_line (start -1.61 -1.61) (end -0.62 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.61 1.61) (end -1.61 1.31) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.61 1.61) (end -0.62 1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.61 1.61) (end 1.61 1.31) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.61 -1.61) (end 1.61 -1.31) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.62 1.61) (end 1.61 1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.62 -1.61) (end 1.61 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.95 -1.95) (end -1.95 1.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.95 -1.95) (end 1.95 -1.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.95 -1.95) (end 1.95 1.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.95 1.95) (end 1.95 1.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -1) (end -1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -1) (end -1 -1.5) (layer F.Fab) (width 0.1))
  (pad "" smd roundrect (at 0 0) (size 1.34 1.55) (layers F.Paste) (roundrect_rratio 0.038))
  (pad "" smd roundrect (at 0.325 -1.337) (size 0.23 0.725) (layers F.Paste) (roundrect_rratio 0.22))
  (pad 9 thru_hole circle (at 0 0.625) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 9 thru_hole circle (at 0 -0.625) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 9 thru_hole circle (at 0.5 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 9 thru_hole circle (at -0.5 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 9 smd roundrect (at 0.325 1.1875) (size 0.23 1.025) (layers F.Cu F.Mask) (roundrect_rratio 0.22))
  (pad 9 smd roundrect (at -0.325 1.1875) (size 0.23 1.025) (layers F.Cu F.Mask) (roundrect_rratio 0.22))
  (pad 4 smd roundrect (at -1.4 0.975) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 3 smd roundrect (at -1.4 0.325) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 2 smd roundrect (at -1.4 -0.325) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 9 smd roundrect (at 0 0) (size 1.5 1.75) (layers F.Cu F.Mask) (roundrect_rratio 0.034))
  (pad 1 smd roundrect (at -1.4 -0.975) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 6 smd roundrect (at 1.4 0.325) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 5 smd roundrect (at 1.4 0.975) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 7 smd roundrect (at 1.4 -0.325) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 8 smd roundrect (at 1.4 -0.975) (size 0.6 0.31) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 9 smd roundrect (at -0.325 -1.1875) (size 0.23 1.025) (layers F.Cu F.Mask) (roundrect_rratio 0.22))
  (pad 9 smd roundrect (at 0.325 -1.1875) (size 0.23 1.025) (layers F.Cu F.Mask) (roundrect_rratio 0.22))
  (pad 9 smd roundrect (at 0 0) (size 1.5 1.75) (layers B.Cu) (roundrect_rratio 0.034))
  (pad "" smd roundrect (at -0.325 -1.337) (size 0.23 0.725) (layers F.Paste) (roundrect_rratio 0.22))
  (pad "" smd roundrect (at 0.325 1.337) (size 0.23 0.725) (layers F.Paste) (roundrect_rratio 0.22))
  (pad "" smd roundrect (at -0.325 1.337) (size 0.23 0.725) (layers F.Paste) (roundrect_rratio 0.22))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_DRB0008A.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
