(module QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm (layer F.Cu) (tedit 5DC5F6A4)
  (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=289), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -4.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm (at 0 4.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.36 -3.11) (end 3.11 -3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.11 -3.11) (end 3.11 -2.36) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.36 3.11) (end -3.11 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.11 3.11) (end -3.11 2.36) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.36 3.11) (end 3.11 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.11 3.11) (end 3.11 2.36) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.36 -3.11) (end -3.11 -3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 -3) (end 3 -3) (layer F.Fab) (width 0.1))
  (fp_line (start 3 -3) (end 3 3) (layer F.Fab) (width 0.1))
  (fp_line (start 3 3) (end -3 3) (layer F.Fab) (width 0.1))
  (fp_line (start -3 3) (end -3 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -3 -2) (end -2 -3) (layer F.Fab) (width 0.1))
  (fp_line (start -3.6 -3.6) (end -3.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.6 3.6) (end 3.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.6 3.6) (end 3.6 -3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.6 -3.6) (end -3.6 -3.6) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -2.8375 -1.95) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -2.8375 -1.3) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -2.8375 -0.65) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -2.8375 0) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -2.8375 0.65) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -2.8375 1.3) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -2.8375 1.95) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -1.95 2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -1.3 2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -0.65 2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at 0 2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at 0.65 2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at 1.3 2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at 1.95 2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at 2.8375 1.95) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at 2.8375 1.3) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at 2.8375 0.65) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at 2.8375 0) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at 2.8375 -0.65) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at 2.8375 -1.3) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at 2.8375 -1.95) (size 1.025 0.3) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at 1.95 -2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 23 smd roundrect (at 1.3 -2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 24 smd roundrect (at 0.65 -2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 25 smd roundrect (at 0 -2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 26 smd roundrect (at -0.65 -2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 27 smd roundrect (at -1.3 -2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 28 smd roundrect (at -1.95 -2.8375) (size 0.3 1.025) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 29 smd rect (at 0 0) (size 4.25 4.25) (layers F.Cu F.Mask))
  (pad "" smd roundrect (at -1.42 -1.42) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at -1.42 0) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at -1.42 1.42) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at 0 -1.42) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at 0 0) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at 0 1.42) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at 1.42 -1.42) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at 1.42 0) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (pad "" smd roundrect (at 1.42 1.42) (size 1.14 1.14) (layers F.Paste) (roundrect_rratio 0.219298))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)