(module DFN-8-1EP_6x5mm_P1.27mm_EP4x4mm (layer F.Cu) (tedit 5EA4BE52)
  (descr "DD Package; 8-Lead Plastic DFN (6mm x 5mm) (see http://www.everspin.com/file/236/download)")
  (tags "dfn ")
  (attr smd)
  (fp_text reference REF** (at 0 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-8-1EP_6x5mm_P1.27mm_EP4x4mm (at 0 3.65) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2 -2.5) (end -3 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3 2.5) (end -3 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3 2.5) (end -3 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3 -2.5) (end 3 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2 -2.5) (end 3 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3.7 2.8) (end -3.7 -2.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.7 2.8) (end -3.7 2.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.7 -2.9) (end 3.7 2.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.7 -2.9) (end 3.7 -2.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -2.6) (end 3 -2.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -3 2.6) (end 3 2.6) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at -2.9 -1.905 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.9 -0.635 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.9 0.635 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.9 1.905 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.9 1.905 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.9 0.635 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.9 -0.635 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.9 -1.905 270) (size 0.5 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0 0 270) (size 4 4) (layers F.Cu F.Mask))
  (pad "" smd rect (at -1.5 -1.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at -0.5 -1.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 0.5 -1.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 1.5 -1.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 1.5 -0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 0.5 -0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at -0.5 -0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at -1.5 -0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 1.5 0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 0.5 0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at -0.5 0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at -1.5 0.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 1.5 1.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at 0.5 1.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at -0.5 1.5 270) (size 0.8 0.8) (layers F.Paste))
  (pad "" smd rect (at -1.5 1.5 270) (size 0.8 0.8) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_6x5mm_Pitch1.27mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
