(module Panasonic_HSON-8_8x8mm_P2.00mm (layer F.Cu) (tedit 5B27E914)
  (descr "Panasonic HSON-8, 8x8x1.25mm (https://industrial.panasonic.com/content/data/SC/ds/ds7/c0/PKG_HSON008-A-0808XXI_EN.pdf)")
  (tags "panasonic hson")
  (solder_mask_margin 0.05)
  (attr smd)
  (fp_text reference REF** (at 0 -5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Panasonic_HSON-8_8x8mm_P2.00mm (at 0 5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3 -4) (end 4 -4) (layer F.Fab) (width 0.1))
  (fp_line (start 4 -4) (end 4 4) (layer F.Fab) (width 0.1))
  (fp_line (start 4 4) (end -4 4) (layer F.Fab) (width 0.1))
  (fp_line (start -4 4) (end -4 -3) (layer F.Fab) (width 0.1))
  (fp_line (start -3 -4) (end -4 -3) (layer F.Fab) (width 0.1))
  (fp_line (start -4.75 -4.25) (end 4.75 -4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.75 -4.25) (end 4.75 4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.75 4.25) (end 4.75 4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.75 4.25) (end -4.75 -4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.11 4.11) (end -4.11 4.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.11 -4.11) (end -4.5 -4.11) (layer F.SilkS) (width 0.12))
  (pad 9 smd rect (at 0.9 0) (size 3.2 6.94) (layers F.Cu F.Mask))
  (pad 1 smd rect (at -3.975 -3) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad "" smd rect (at -4 -3) (size 1 1.3) (layers F.Paste))
  (pad "" smd rect (at -4 -1) (size 1 1.3) (layers F.Paste))
  (pad "" smd rect (at -4 1) (size 1 1.3) (layers F.Paste))
  (pad "" smd rect (at -4 3) (size 1 1.3) (layers F.Paste))
  (pad "" smd rect (at 4 3) (size 1 1.3) (layers F.Paste))
  (pad "" smd rect (at 4 1) (size 1 1.3) (layers F.Paste))
  (pad "" smd rect (at 4 -1) (size 1 1.3) (layers F.Paste))
  (pad "" smd rect (at 4 -3) (size 1 1.3) (layers F.Paste))
  (pad 2 smd rect (at -3.975 -1) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad 3 smd rect (at -3.975 1) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad 4 smd rect (at -3.975 3) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad 5 smd rect (at 3.975 3) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad 6 smd rect (at 3.975 1) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad 7 smd rect (at 3.975 -1) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad 8 smd rect (at 3.975 -3) (size 1.05 1.3) (layers F.Cu F.Mask))
  (pad "" smd rect (at 0.15 -1.5) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 1.65 -1.5) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 0.15 0) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 1.65 0) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 0.15 1.5) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 1.65 1.5) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 0.15 3) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 1.65 3) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 0.15 -3) (size 0.9 0.9) (layers F.Paste))
  (pad "" smd rect (at 1.65 -3) (size 0.9 0.9) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Panasonic_HSON-8_8x8mm_P2.00mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
