(module SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5A0AA2C1)
  (descr "20-Lead Plastic Quad Flat, No Lead Package - 3x3 mm Body [QFN] with corner pads; see figure 8.2 of https://www.silabs.com/documents/public/data-sheets/efm8bb1-datasheet.pdf")
  (tags "QFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (at 0 3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.65 0.65) (thickness 0.125)))
  )
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 1.5) (end -1.5 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -0.5) (end -0.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.25 -2.25) (end -2.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.25 2.25) (end 2.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.25 2.25) (end 2.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.25 -2.25) (end -2.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.16 -1.66) (end 1.66 -1.66) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.66 -1.66) (end 1.66 -1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.16 1.66) (end -1.66 1.66) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.66 1.66) (end -1.66 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.16 1.66) (end 1.66 1.66) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.66 1.66) (end 1.66 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.66 -1.66) (end -1.16 -1.66) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at -1.25 -1.25) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.55 -0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.55 -0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.55 0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.55 0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.25 1.25) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -0.75 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -0.25 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.25 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.75 1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.25 1.25) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.55 0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 1.55 0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.55 -0.25) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 1.55 -0.75) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 1.25 -1.25) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 0.75 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 0.25 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -0.25 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -0.75 -1.55 90) (size 0.9 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 0 0) (size 1.8 1.8) (layers F.Cu F.Mask))
  (pad "" smd rect (at -0.45 -0.45) (size 0.54 0.54) (layers F.Paste))
  (pad "" smd rect (at -0.45 0.45) (size 0.54 0.54) (layers F.Paste))
  (pad "" smd rect (at 0.45 -0.45) (size 0.54 0.54) (layers F.Paste))
  (pad "" smd rect (at 0.45 0.45) (size 0.54 0.54) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
