(module Texas_R_PUQFN-N12 (layer F.Cu) (tedit 5A0AA2C1)
  (descr "Texas_R_PUQFN-N12 http://www.ti.com/lit/ds/symlink/txb0104.pdf")
  (tags Texas_R_PUQFN-N12)
  (attr smd)
  (fp_text reference REF** (at 0.75 -2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_R_PUQFN-N12 (at 0.25 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.03)))
  )
  (fp_line (start 0.6 -1.3) (end -1.09 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.5 1.3) (end -0.5 1.3) (layer F.SilkS) (width 0.1))
  (fp_line (start 1.1 1.2) (end -1.1 1.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.1 1.2) (end -1.1 -1.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.1 -1.2) (end 1.1 -1.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.1 -1.2) (end 1.1 1.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 -1) (end -0.85 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0.85 -1) (end 0.85 1) (layer F.Fab) (width 0.1))
  (fp_line (start 0.85 1) (end -0.85 1) (layer F.Fab) (width 0.1))
  (fp_line (start -0.85 1) (end -0.85 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1) (end 0.85 -1) (layer F.Fab) (width 0.1))
  (pad 1 smd rect (at -0.65 -0.8 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.65 -0.4 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.65 0 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.65 0.4 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.65 0.8 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0 0.8 270) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.65 0.8 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.65 0.4 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.65 0 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.65 -0.4 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0.65 -0.8 270) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 0 -0.8 270) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.425 -0.975) (size 0.15 0.25) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_R_PUQFN-N12.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
