(module Texas_X2QFN-12_1.6x1.6mm_P0.4mm (layer F.Cu) (tedit 5D9F792E)
  (descr "Texas  X2QFN, 12 Pin (http://www.ti.com/lit/ml/mpqf391c/mpqf391c.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "Texas X2QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_X2QFN-12_1.6x1.6mm_P0.4mm (at 0 2.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.91 -0.91) (end 0.91 -0.56) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.91 0.91) (end -0.91 0.56) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.91 0.91) (end 0.91 0.56) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.4 -0.8) (end 0.8 -0.8) (layer F.Fab) (width 0.1))
  (fp_line (start 0.8 -0.8) (end 0.8 0.8) (layer F.Fab) (width 0.1))
  (fp_line (start 0.8 0.8) (end -0.8 0.8) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 0.8) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 -0.4) (end -0.4 -0.8) (layer F.Fab) (width 0.1))
  (fp_line (start -1.4 -1.4) (end -1.4 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.4 1.4) (end 1.4 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.4 1.4) (end 1.4 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.4 -1.4) (end -1.4 -1.4) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -0.725 -0.2) (size 0.85 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -0.725 0.2) (size 0.85 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -0.6 0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -0.2 0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 0.2 0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 0.6 0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 0.725 0.2) (size 0.85 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 0.725 -0.2) (size 0.85 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 0.6 -0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 0.2 -0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -0.2 -0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -0.6 -0.825) (size 0.2 0.65) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.4 0.4) (thickness 0.06)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_X2QFN-12_1.6x1.6mm_P0.4mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)