(module UDFN-9_1.0x3.8mm_P0.5mm (layer F.Cu) (tedit 5EA4C19E)
  (descr "9-pin UDFN package, 1.0x3.8mm, (Ref: https://katalog.we-online.de/pbs/datasheet/824014881.pdf)")
  (tags "UDFN SMD")
  (attr smd)
  (fp_text reference REF** (at 0 -2.9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value UDFN-9_1.0x3.8mm_P0.5mm (at 0 2.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.5 -1.9) (end -0.1 -1.9) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1.5) (end -0.5 1.9) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 1.9) (end 0.5 1.9) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 1.9) (end 0.5 -1.9) (layer F.Fab) (width 0.1))
  (fp_line (start -0.1 -1.9) (end -0.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0.65 -1.65) (end 0.65 -2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.65 -2.05) (end 0 -2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.65 1.65) (end 0.65 2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.65 2.05) (end -0.55 2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.65 -0.05) (end 0.65 0.05) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.65 0.35) (end -0.65 0.45) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.65 0.75) (end 0.65 0.95) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.65 1.15) (end -0.65 1.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.65 -0.45) (end -0.65 -0.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.65 -0.95) (end 0.65 -0.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.03 -2.15) (end -1.03 -2.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.03 -2.15) (end -1.03 2.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.03 2.15) (end 1.03 2.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.03 2.15) (end 1.03 -2.15) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0 90) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.05)))
  )
  (pad 1 smd rect (at -0.475 -1.7) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.475 -0.8) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.475 0) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.475 0.8) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.475 1.7) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.475 1.3) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.475 0.4) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.475 -0.4) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.475 -1.3) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UDFN-9_1.0x3.8mm_P0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
