(module DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm (layer F.Cu) (tedit 5EA4BDEC)
  (descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
  (tags "DFN 0.65")
  (attr smd)
  (fp_text reference REF** (at 0 -2.55) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm (at 0 2.55) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.75 1.4) (end 2.13 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 1.75) (end 1.75 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.56 1.56) (end 1.56 1.41) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.105)))
  )
  (fp_line (start -0.75 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 1.5) (end -1.5 -0.75) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -0.75) (end -0.75 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.13 -1.4) (end 2.13 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 1.75) (end 1.75 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.56 1.56) (end 1.56 1.56) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -1.56) (end 1.56 -1.56) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.56 1.56) (end -1.56 1.41) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.56 -1.56) (end 1.56 -1.41) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.75 -1.4) (end 2.13 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 -1.75) (end 1.75 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -1.75) (end -1.75 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -1.4) (end -2.13 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.13 -1.4) (end -2.13 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 1.4) (end -2.13 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 1.75) (end -1.75 1.4) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -1.55 -0.975) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.55 -0.325) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.55 0.325) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.55 0.975) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.55 0.975) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.55 0.325) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.55 -0.325) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.55 -0.975) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
  (pad "" smd rect (at -0.3875 0.6) (size 0.6 1) (layers F.Paste))
  (pad 9 smd rect (at 0 0) (size 1.55 2.4) (layers F.Cu F.Mask))
  (pad "" smd rect (at 0.3875 0.6) (size 0.6 1) (layers F.Paste))
  (pad "" smd rect (at 0.3875 -0.6) (size 0.6 1) (layers F.Paste))
  (pad "" smd rect (at -0.3875 -0.6) (size 0.6 1) (layers F.Paste))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
