(module UQFN-20_3x3mm_P0.4mm (layer F.Cu) (tedit 5F6D1AD2)
  (descr "UQFN, 20 Pin (https://resurgentsemi.com/wp-content/uploads/2018/09/MPR121_rev5-Resurgent.pdf?d453f8&d453f8), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "UQFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value UQFN-20_3x3mm_P0.4mm (at 0 2.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.16 -1.61) (end 1.61 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.61 -1.61) (end 1.61 -1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.16 1.61) (end -1.61 1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.61 1.61) (end -1.61 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.16 1.61) (end 1.61 1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.61 1.61) (end 1.61 1.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.16 -1.61) (end -1.61 -1.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 1.5) (end -1.5 -0.75) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -0.75) (end -0.75 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.1 -2.1) (end -2.1 2.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.1 2.1) (end 2.1 2.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.1 2.1) (end 2.1 -2.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.1 -2.1) (end -2.1 -2.1) (layer F.CrtYd) (width 0.05))
  (pad 1 smd custom (at -1.3875 -0.8) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4225 -0.06) (xy 0.325931 -0.06) (xy 0.4225 0.036569) (xy 0.4225 0.06)
         (xy -0.4225 0.06)) (width 0.08))
    ))
  (pad 2 smd roundrect (at -1.3875 -0.4) (size 0.925 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.3875 0) (size 0.925 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -1.3875 0.4) (size 0.925 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd custom (at -1.3875 0.8) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4225 -0.06) (xy 0.4225 -0.06) (xy 0.4225 -0.036569) (xy 0.325931 0.06)
         (xy -0.4225 0.06)) (width 0.08))
    ))
  (pad 6 smd custom (at -0.8 1.3875) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.06 -0.325931) (xy 0.036569 -0.4225) (xy 0.06 -0.4225) (xy 0.06 0.4225)
         (xy -0.06 0.4225)) (width 0.08))
    ))
  (pad 7 smd roundrect (at -0.4 1.3875) (size 0.2 0.925) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 0 1.3875) (size 0.2 0.925) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 0.4 1.3875) (size 0.2 0.925) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd custom (at 0.8 1.3875) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.06 -0.4225) (xy -0.036569 -0.4225) (xy 0.06 -0.325931) (xy 0.06 0.4225)
         (xy -0.06 0.4225)) (width 0.08))
    ))
  (pad 11 smd custom (at 1.3875 0.8) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4225 -0.06) (xy 0.4225 -0.06) (xy 0.4225 0.06) (xy -0.325931 0.06)
         (xy -0.4225 -0.036569)) (width 0.08))
    ))
  (pad 12 smd roundrect (at 1.3875 0.4) (size 0.925 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at 1.3875 0) (size 0.925 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at 1.3875 -0.4) (size 0.925 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 15 smd custom (at 1.3875 -0.8) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4225 0.036569) (xy -0.325931 -0.06) (xy 0.4225 -0.06) (xy 0.4225 0.06)
         (xy -0.4225 0.06)) (width 0.08))
    ))
  (pad 16 smd custom (at 0.8 -1.3875) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.06 -0.4225) (xy 0.06 -0.4225) (xy 0.06 0.325931) (xy -0.036569 0.4225)
         (xy -0.06 0.4225)) (width 0.08))
    ))
  (pad 17 smd roundrect (at 0.4 -1.3875) (size 0.2 0.925) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at 0 -1.3875) (size 0.2 0.925) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at -0.4 -1.3875) (size 0.2 0.925) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 20 smd custom (at -0.8 -1.3875) (size 0.115147 0.115147) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.06 -0.4225) (xy 0.06 -0.4225) (xy 0.06 0.4225) (xy 0.036569 0.4225)
         (xy -0.06 0.325931)) (width 0.08))
    ))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.75 0.75) (thickness 0.11)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-20_3x3mm_P0.4mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)