(module Texas_VSON-HR-8_1.5x2mm_P0.5mm (layer F.Cu) (tedit 5DC5F54E)
  (descr "Texas  VSON-HR, 8 Pin (http://www.ti.com/lit/ds/symlink/tps62823.pdf#page=29), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "Texas VSON-HR NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -1.95) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_VSON-HR-8_1.5x2mm_P0.5mm (at 0 1.95) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -1.11) (end 0.75 -1.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 1.11) (end 0.75 1.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.375 -1) (end 0.75 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 0.75 -1) (end 0.75 1) (layer F.Fab) (width 0.1))
  (fp_line (start 0.75 1) (end -0.75 1) (layer F.Fab) (width 0.1))
  (fp_line (start -0.75 1) (end -0.75 -0.625) (layer F.Fab) (width 0.1))
  (fp_line (start -0.75 -0.625) (end -0.375 -1) (layer F.Fab) (width 0.1))
  (fp_line (start -1.38 -1.25) (end -1.38 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.38 1.25) (end 1.38 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.38 1.25) (end 1.38 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.38 -1.25) (end -1.38 -1.25) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -0.725 -0.75) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -0.725 -0.25) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -0.725 0.25) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -0.725 0.75) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 0.725 0.75) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 0.725 0.25) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 0.725 -0.25) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 0.725 -0.75) (size 0.8 0.25) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.38 0.38) (thickness 0.06)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_VSON-HR-8_1.5x2mm_P0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)