(module Texas_VQFN-RHL-20 (layer F.Cu) (tedit 5B833432)
  (descr http://www.ti.com/lit/ds/symlink/bq51050b.pdf)
  (tags RHL0020A)
  (attr smd)
  (fp_text reference REF** (at 0 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Texas_VQFN-RHL-20 (at 0 3.7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -3.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.9 -2.3) (end -1 -2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.8 2) (end -1.8 2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.8 2.3) (end -1 2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.8 2) (end 1.8 2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.8 -2.3) (end 1.8 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 2.3) (end 1.8 2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 -2.3) (end 1.8 -2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.2 -2.7) (end -2.2 2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.2 -2.7) (end 2.2 -2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.2 -2.7) (end 2.2 2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.2 2.7) (end 2.2 2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.23 -2.25) (end 1.75 -2.25) (layer F.Fab) (width 0.1))
  (fp_line (start 1.75 -2.25) (end 1.75 2.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.75 2.25) (end 1.75 2.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.75 -1.73) (end -1.75 2.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.75 -1.73) (end -1.23 -2.25) (layer F.Fab) (width 0.1))
  (pad "" smd rect (at 0 1.8) (size 0.75 0.25) (layers F.Paste))
  (pad "" smd rect (at 0 -1.8) (size 0.75 0.25) (layers F.Paste))
  (pad "" smd rect (at 0.56 1.05) (size 0.92 0.85) (layers F.Paste))
  (pad "" smd rect (at -0.56 1.05) (size 0.92 0.85) (layers F.Paste))
  (pad "" smd rect (at 0.56 0) (size 0.92 0.85) (layers F.Paste))
  (pad "" smd rect (at -0.56 0) (size 0.92 0.85) (layers F.Paste))
  (pad "" smd rect (at 0.56 -1.05) (size 0.92 0.85) (layers F.Paste))
  (pad "" smd rect (at -0.56 -1.05) (size 0.92 0.85) (layers F.Paste))
  (pad 21 smd roundrect (at 0.275 2.15) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at -0.275 2.15) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at 0.275 -2.15) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at -0.275 -2.15) (size 0.2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at 0.75 -2.15) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 19 smd roundrect (at 1.65 -1.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 18 smd roundrect (at 1.65 -1.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 17 smd roundrect (at 1.65 -0.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 16 smd roundrect (at 1.65 -0.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 15 smd roundrect (at 1.65 0.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 14 smd roundrect (at 1.65 0.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 13 smd roundrect (at 1.65 1.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 12 smd roundrect (at 1.65 1.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 11 smd roundrect (at 0.75 2.15) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 10 smd roundrect (at -0.75 2.15) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 9 smd roundrect (at -1.65 1.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 8 smd roundrect (at -1.65 1.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 7 smd roundrect (at -1.65 0.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 6 smd roundrect (at -1.65 0.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 5 smd roundrect (at -1.65 -0.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 4 smd roundrect (at -1.65 -0.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 3 smd roundrect (at -1.65 -1.25) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 2 smd roundrect (at -1.65 -1.75) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 1 smd roundrect (at -0.75 -2.15) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.21))
  (pad 21 smd custom (at 0 0) (size 1.524 1.524) (layers F.Cu F.Mask)
    (zone_connect 0)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 1.025 1.525) (xy 1.025 -1.525) (xy 0.375 -1.525) (xy 0.375 -1.925) (xy -0.375 -1.925)
         (xy -0.375 -1.525) (xy -1.025 -1.525) (xy -1.025 1.525) (xy -0.375 1.525) (xy -0.375 1.925)
         (xy 0.375 1.925) (xy 0.375 1.525)) (width 0))
    ))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_VQFN-RHL-20_ThermalVias.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
