(module UQFN-10_1.3x1.8mm_P0.4mm (layer F.Cu) (tedit 5D9F792E)
  (descr "UQFN, 10 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/00001725D.pdf (Page 9)), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "UQFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value UQFN-10_1.3x1.8mm_P0.4mm (at 0 2.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.76 -1.01) (end 0.76 -0.56) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.76 1.01) (end -0.76 0.56) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.76 1.01) (end 0.76 0.56) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.325 -0.9) (end 0.65 -0.9) (layer F.Fab) (width 0.1))
  (fp_line (start 0.65 -0.9) (end 0.65 0.9) (layer F.Fab) (width 0.1))
  (fp_line (start 0.65 0.9) (end -0.65 0.9) (layer F.Fab) (width 0.1))
  (fp_line (start -0.65 0.9) (end -0.65 -0.575) (layer F.Fab) (width 0.1))
  (fp_line (start -0.65 -0.575) (end -0.325 -0.9) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 -1.5) (end -1.25 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.25 1.5) (end 1.25 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.25 1.5) (end 1.25 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.25 -1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -0.6 -0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -0.6 0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -0.4 0.875) (size 0.2 0.75) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 0 0.875) (size 0.2 0.75) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 0.4 0.875) (size 0.2 0.75) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 0.6 0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 0.6 -0.2) (size 0.8 0.2) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 0.4 -0.875) (size 0.2 0.75) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 0 -0.875) (size 0.2 0.75) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -0.4 -0.875) (size 0.2 0.75) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.25))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.32 0.32) (thickness 0.05)))
  )
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-10_1.3x1.8mm_P0.4mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)