(module Diodes_UDFN2020-6_Type-F (layer F.Cu) (tedit 5F0E175D)
  (descr "U-DFN2020-6 (Type F) (https://www.diodes.com/assets/Package-Files/U-DFN2020-6-Type-F.pdf) ")
  (tags "U-DFN2020-6 (Type F)")
  (attr smd)
  (fp_text reference REF** (at 0 -2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Diodes_UDFN2020-6_Type-F (at 0 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0.1) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.05)))
  )
  (fp_line (start -0.5 -1) (end -1 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1 1) (end -1 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1 1) (end -1 1) (layer F.Fab) (width 0.1))
  (fp_line (start 1 -1) (end 1 1) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1) (end 1 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 1 -1.15) (end 0 -1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 1.15) (end -1 1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.4 1.25) (end 1.4 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.4 1.25) (end 1.4 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.4 -1.25) (end -1.4 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.4 -1.25) (end -1.4 -1.25) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -0.9375 -0.65) (size 0.425 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.9375 0) (size 0.425 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.9375 0.65) (size 0.425 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.9375 0.65) (size 0.425 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.9375 0) (size 0.425 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.9375 -0.65) (size 0.425 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0 -0.325) (size 1.15 0.95) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0 0.7) (size 0.8 0.48) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Diodes_UDFN2020-6_Type-F.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
