(module ROHM_DFN0604-3 (layer F.Cu) (tedit 5A0AA2C1)
  (descr "DFN package size 0604 3 pins")
  (tags "DFN package size 0604 3 pins")
  (attr smd)
  (fp_text reference REF** (at 0 -1.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ROHM_DFN0604-3 (at 0 1.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -1.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.45 -0.4) (end -0.45 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.4 -0.4) (end -0.45 -0.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -0.4) (end -0.4 -0.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.55 0.53) (end -0.55 -0.53) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.55 0.53) (end -0.55 0.53) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.55 -0.53) (end 0.55 0.53) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.55 -0.53) (end 0.55 -0.53) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.3 -0.2) (end 0.3 -0.2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.3 0.2) (end -0.3 -0.2) (layer F.Fab) (width 0.1))
  (fp_line (start 0.3 0.2) (end -0.3 0.2) (layer F.Fab) (width 0.1))
  (fp_line (start 0.3 -0.2) (end 0.3 0.2) (layer F.Fab) (width 0.1))
  (pad 1 smd rect (at -0.195 -0.15 270) (size 0.25 0.27) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.195 0.15 270) (size 0.25 0.27) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.155 0 270) (size 0.35 0.35) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/ROHM_DFN0604-3.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
